IMPACT LET: Solar Energetic Particle Intensities

Overview

The Low Energy Telescope (LET) is one of four sensors that make up the Solar Energetic Particle (SEP) instrument of the IMPACT investigation for NASA's STEREO mission. LET consists of a sensor system made up of an array of 14 solid-state detectors composed of 54 segments that are individually analyzed by custom Pulse Height Analysis System Integrated Circuits (PHASICs). The signals from four PHASIC chips in each LET are used by a Minimal Instruction Set Computer (MISC) to provide on-board particle identification of energetic particles from H through Ni in ~12 energy intervals at event rates of up to ~1000 events/sec.

The primary measurement goal of the LET instrument is to measure the composition, energy spectra, and time variations of solar energetic particles ranging from H to Ni. The energy range for oxygen extends from ∼3 to 30 MeV/nucleon. Detailed documentation of the instrument design and science goals may be found in the instrument paper published in Space Science Reviews (SSR): Space Sci Rev (2008) 136: 285–3 ( <https://doi.org/10.1007/s11214-007-9288-x> ).




Figure 1: LET Instrument Cross-Section




Figure 2: LET Instrument Species and Energy-range

Heritage

The LET instrument employs the well-established dE/dx vs. total energy technique to determine the nuclear charge, and in some cases the mass, of detected heavy ions. This particle identification technique uses the energy loss signal from a detector that the particle fully penetrates (ΔE) and the energy deposited in a following detector in which the particle stops (E'), together with the thickness penetrated in the ΔE detector (L) to obtain an estimate of the particle’s charge, Z. The technique has been used in many previous instruments, e.g. the SIS instrument on ACE, the CRS subsystem on Voyager, etc. The technique is described in detail in the SSR instrument paper, as is the implementation of this technique in the onboard particle identification system.

Instrument Data Acquisition and Onboard Data Processing Features

Dynamic Thresholds

An important feature of the onboard data acquisition is the “dynamic threshold” system. During large SEP events the single-detector count rates can increase by a factor of as much as 104, due mostly to low-energy protons. These elevated single-detector count rates create instrument dead-time and can also lead to chance coincidence events involving two separate particles. In order to minimize these effects, the LET design includes “dynamic thresholds” in which the trigger threshold on selected PHAs are increased during periods when the count rates are high. This action reduces the count rates of selected detectors, minimizing dead-time and effectively reducing the geometry factor for H and He events with minimal effect on the geometry factor for heavy ions with Z ≥ 6.

The dynamic threshold state of the instrument is included in the raw telemetry and is required for conversion of the raw data to physical units. A detailed description of the dynamic threshold system is included in this document as an appendix.

Onboard Particle Identification and Energy/Sector Binning

See Appendix D, Section 2.4.

Level 1 and Level 2 Data Products Description

The LET Level 1 and Level 2 data are energetic particle intensities (1/(cm^2 s sr MeV/nuc)) for 16 species, in ~12 energy-bins per species.

The Level 1 and Level 2 data are derived from the science and look-direction rates in the instrument telemetry data. These rates are described in detail in Appendix D, sections 2.4 and 2.5.

The highest time-resolution data provided by LET is 1 minute (Level 1 data). The LET 1-minute data are available in CDF format from the [STEREO IMPACT Data portal at Berkeley](http://sprg.ssl.berkeley.edu/impact/data_index.html), and from [CDAWeb](https://cdaweb.gsfc.nasa.gov/index.html/).

We also provide Level 2 data, which are 10-minute averaged, hourly-averaged, daily-averaged, and 27-day averaged data, derived directly from the 1-minute Level 1 data. These Level 2 data are in ASCII text files, with each file containing one calendar year of data, for one species, for one spacecraft. For the 10-minute averages, we also provide files containing 1 month of data.

Each ASCII file begins with a header that provides version and other provenance information and describes each data field.

The LET Level 1 and Level 2 data are available in three "flavors": Standard, Summed, and Sectored:

* **Standard**: Includes intensities for all the species/energy combinations defined in the LET onboard software. Some of the species/energy combinations may be set to FILL-DATA, as described in the release-notes/caveats. The latest release-notes/caveats are included in this document as an appendix.
* **Summed**: For each species the standard energy-bins are combined into wider energy-bins. These wider bins have better statistics and are common to most/all of the species identified by LET. These Summed data are useful for calculating element ratios and may be more useful than the Standard data during quiet periods.
* **Sectored**: The LET onboard software sorts events into 16 look-directions, or sectors (See figure 3), 8 per side. Both the front (A-side) and rear (B-side) include particles from a 129deg x 29deg Field of View (FOV) with the 129deg fan looking along the ecliptic plane. The center of the A-side 129deg fan points at an angle that is 45deg from the Sun-spacecraft line. When the spacecraft is in its nominal roll orientation, this direction is 45deg west of the Sun (along the average Parker Spiral direction at 1 AU), i.e., in the [-R,+T] direction. Since July 2015, after solar conjunction, the two STEREO spacecraft have been rolled 180deg about the Sun-spacecraft line in order to allow the high gain antenna to remain pointing at Earth. Consequently, the center of the A-side fan now points 45deg east of the Sun, in the [-R,-T] direction (i.e., perpendicular to the average Parker Spiral direction). Except for brief periods when the spacecraft is rolled for SECCHI or MAG calibrations, this will remain the case until the spacecraft passes by Earth again in 2023. Periods of off-nominal roll angles (including those at the beginning of the mission, when the spacecraft were still in Earth orbit) are shown in the plots at <http://www.srl.caltech.edu/STEREO/PLOTS/LET/AnisoPlots/pointingplot.pdf>

For the sectored data in particular, it is important to understand the orientation of the LET instrument on the spacecraft, and the methods for calculating spacecraft attitude and roll angle. Detailed information for doing this is included in this document as an appendix.




Figure 3: The LET viewing directions are divided into 8 sectors on the A-side and 8 on the B-side. Shown here is the fraction of the geometry factor in each sector on the A-side. In this representation the particles coming in a straight line from the Sun would arrive at 0 degrees and those arriving along the average Parker spiral angle would arrive at ~45 degrees. Note that the central six sectors are 12.5 degrees wide and the width of the two outside sectors is 25 degrees.

Full Listing of Standard Species/Energy Bins in the LET Level 1 and Level 2 data

H)

1.8 - 2.2 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

2.2 - 2.7 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

2.7 - 3.2 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

3.2 - 3.6 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

He3)

2.2 - 2.7 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

2.7 - 3.2 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

3.2 - 3.6 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

He4)

1.8 - 2.2 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

2.2 - 2.7 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

2.7 - 3.2 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

3.2 - 3.6 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

He)

2.2 - 2.7 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

2.7 - 3.2 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

3.2 - 3.6 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

C)

3.2 - 3.6 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

N)

3.2 - 3.6 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

O)

3.2 - 3.6 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

Ne)

3.2 - 3.6 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

Na)

6.0 - 8.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

Mg)

3.2 - 3.6 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

40.0 - 52.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

Al)

6.0 - 8.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

40.0 - 52.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

Si)

3.2 - 3.6 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

40.0 - 52.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

S)

3.6 - 4.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

40.0 - 52.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

Ar)

3.6 - 4.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

40.0 - 52.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

Ca)

3.6 - 4.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

40.0 - 52.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

Fe)

2.7 - 3.2 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

3.2 - 3.6 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

3.6 - 4.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 4.5 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

4.5 - 5.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

5.0 - 6.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 8.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

8.0 - 10.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

40.0 - 52.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

52.0 - 70.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

Ni)

8.0 - 10.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 12.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

12.0 - 15.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 21.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

21.0 - 27.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 33.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

33.0 - 40.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

40.0 - 52.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

52.0 - 70.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

Full Listing of Summed Species/Energy Bins in the LET Level 1 and Level 2 data

H)

1.8 - 3.6 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 6.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV proton intensity (1/(cm^2 s sr MeV/nuc))

He3)

4.0 - 6.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n 3He intensity (1/(cm^2 s sr MeV/nuc))

He4)

1.8 - 3.6 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

4.0 - 6.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n 4He intensity (1/(cm^2 s sr MeV/nuc))

He)

4.0 - 6.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n He intensity (1/(cm^2 s sr MeV/nuc))

C)

4.0 - 6.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n carbon intensity (1/(cm^2 s sr MeV/nuc))

N)

4.0 - 6.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n nitrogen intensity (1/(cm^2 s sr MeV/nuc))

O)

4.0 - 6.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n oxygen intensity (1/(cm^2 s sr MeV/nuc))

Ne)

4.0 - 6.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n neon intensity (1/(cm^2 s sr MeV/nuc))

Na)

10.0 - 15.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n sodium intensity (1/(cm^2 s sr MeV/nuc))

Mg)

4.0 - 6.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n magnesium intensity (1/(cm^2 s sr MeV/nuc))

Al)

6.0 - 10.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n aluminum intensity (1/(cm^2 s sr MeV/nuc))

Si)

4.0 - 6.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 40.0 MeV/n silicon intensity (1/(cm^2 s sr MeV/nuc))

S)

4.0 - 6.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 40.0 MeV/n sulfur intensity (1/(cm^2 s sr MeV/nuc))

Ar)

4.0 - 6.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 40.0 MeV/n argon intensity (1/(cm^2 s sr MeV/nuc))

Ca)

4.0 - 6.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 40.0 MeV/n calcium intensity (1/(cm^2 s sr MeV/nuc))

Fe)

4.0 - 6.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

6.0 - 10.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

10.0 - 15.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 40.0 MeV/n iron intensity (1/(cm^2 s sr MeV/nuc))

Ni)

10.0 - 15.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

15.0 - 27.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

27.0 - 40.0 MeV/n nickel intensity (1/(cm^2 s sr MeV/nuc))

Full Listing of Sectored Species/Energy Bins in the LET Level 1 and Level 2 data

After Nov 22, 2010, the sectored rates are assigned as follows:

0 - 15: H 4-6 MeV/nuc

15 - 31: H 1.8-3.6

32 - 47: 4He 4-6

48 - 63: 4He 6-12

64 - 79: CNO 4-6

80 - 95: CNO 6-12

96 - 111: NeMgSi 4-6

112 - 127: NeMgSi 6-12

128 - 143: Fe 4-12

144 - 159: H 6-10

Prior to Nov 22, 2010 the sectored rates were:

0 - 15: H 4-6 MeV/nuc

15 - 31: 3He 4-6

32 - 47: 4He 4-6

48 - 63: 4He 6-12

64 - 79: CNO 4-6

80 - 95: CNO 6-12

96 - 111: NeMgSi 4-6

112 - 127: NeMgSi 6-12

128 - 143: Fe 4-6

144 - 159: Fe 6-12

Theoretical Description

The conversion from raw counts to energetic particle intensities uses the following simple formula:

* The raw data are counts (compressed), for N species, M energy bins, X look-directions. For STEREO/LET, N=16, M~12, X=16
* The physical quantity is Flux(N,M,X) (also called Intensity),

Where Flux(N,M,X) = counts(N,M,X)/Z,

Where Z = Livetime \* Ebin\_width(N,M,X) \* Geom(N,M,X) \*Eff(N,M,X)

**Ebin\_width** is the width of the energy bin, in MeV/nucleon.

**Geom** is the Geometry factor (see Appendix E). During large SEP events, the geometry factors for H and He depend upon the dynamic-threshold state of the instrument. This dynamic-threshold state is included in each record in the LET data and is used in the Level 1 data processing to select the appropriate geometry factor when computing the intensities.

Appropriate geometry factors for each dynamic-threshold state are included in the calibration files.

**Eff** is an efficiency factor, which is usually 1.0.

The steps involved in the computation of the intensities are:

* Read calibration data (Ebin\_width, Geom, Eff arrays)
  + Note: these calibration data are time-dependent (at least several discreet changes during the mission, mostly early in the mission)
* Unpack data from CCSDS packets
* Read Livetime and dynamic-threshold state
* Decompress counts data - counts(N,M,X)
* Compute Flux(N,M,X)

The rates decompression is described in Appendix D.

The calibration data (Ebin\_width, Geom, Eff arrays) are stored in ascii tables, and a separate table contains information about which calibration files to read based on the date/time of the data being processed.

The IDL code and associated calibration files that implement the above algorithm are available online from the STEREO IMPACT website at <https://sprg.ssl.berkeley.edu/impact/peters/level1_software/>

Error Analysis and Corrections

Uncertainties due to Counting Statistics

The Level 1 and Level 2 data contain the raw counts for item in the data products, for each time interval. The uncertainties due to counting statistics may be calculated by the user from these counts data.

Systematic Uncertainties

**A.2.6.2.1: Detector Thicknesses and Uniformity.**

Precise measurements of elemental and isotopic abundances require precise knowledge of thickness variations in the L1 and L2 detectors (L1 nominal thickness = 24 microns; L2 nominal thickness = 50 microns). Each of the ten L1 detectors has three segments. Each of two L2 detectors has 10 segments. Prior to final assembly thickness maps were made of all L1 detectors (3 equal-area segments) and L2 Detectors (10 equal-area segments). These maps were made with a collimated beam of 8.78 MeV alpha particles from a radioactive Th228 source. The most uniform devices were selected for flight. (Thermal vacuum data also played a role in detector selection.) Additional information on the L1, L2, and L3 thickness variations was available from accelerator data at the Michigan State University Cyclotron. The mean thicknesses of all LET L1 detectors in the LET-1 and LET-2 instruments are summarized in in Table 17 of the LET Instrument Paper in Space Science Reviews (Mewaldt et al. 2008). The thickness maps and trajectory corrections make it possible to do onboard identification of H, He, C, N, O, Ne, Mg, Si, S, Ar, Ca, Fe, and Ni, as well as 3He and 4He. The mass resolution of He in LET is 0.23 amu in Range 2 and 0.20 amu in Range 3.

**A.2.6.2.2: Chance Coincidences**

The segmentation of the L1, L2, and L3 detectors provides some protection against chance coincidences of two separate particles simulating a single event because it often will result in multiple hits in one of the layers. Range 3 ions will produce two independent measurements of the charge and energy which should agree. These checks can be made during ground processing. These issues are greater for electrons which often do not result in straight-line trajectories.

**A.2.6.2.3: Live-time Effects**

In the largest SEP events such as the July 23, 2012 event the live-time reported in telemetry by the flight software may be in error because of the extremely high count rates.

The onboard livetime counter records the amount of time that the instrument is waiting for a trigger. As soon as it gets a trigger, it system enters a coincidence window where it waits to see if any other detectors were hit. During this time, however, an independent event COULD get in and be analyzed by the instrument, even though the livetime counter does not recognize any portion of the coincidence window as "live". That is, to get the "proper" livetime, we need to add to the measured livetime the length of the coincidence window (or at least some fraction of it) for every instrument trigger. Since we record the number of triggers, NUMTRIG, this means we want:

NewLiveTime = Livetime + N \* NUMTRIG,

where N is the length of time per trigger to be added.

N can be determined for LET by making use of the “livestim” data, which are events generated onboard by electronic pulses, and provide an independent measure of the livetime. Comparison of the livestim data with the reported livetime counter indicates that N = 0.9 microseconds.

In 2013, the Level 1 data processing software for LET was updated to implement this livetime correction, and the LET data from the start of the mission were reprocessed and rereleased on April 3, 2013 (See the Release Notes).

**A.2.6.2.4: Cross Calibration of the LET and HET Sensors with GOES and IMP-8**

During December 2006 there was a series of large SEP events shortly after the launch of STEREO A&B. This period provided a rare opportunity to cross calibrate the STEREO LET & HET sensors with GOES. The first results of this cross calibration were presented in Mewaldt et al. (2015). They showed reasonable agreement for >10 MeV peak intensities and fluences. Subsequently Rodriguiz et al. (2017) cross-calibrated the proton response of GOES xx with both IMP-8 and STEREO A&B. The comparison showed that the GOES-15 was systematically overestimating proton intensities at higher energies (e.g., by x1.7 for >30 MeV; x2.1 for >60 MeV and x2.7 for >100 MeV protons. The results of this study also demonstrate good consistency between the two long-term IMP-8 GME and STEREO LET and HET solar proton data sets.

**A.2.6.2.4: Quantifying the Systematic Uncertainties**

Quantifying the contribution of these characteristics to a set of systematic errors is difficult. Some estimate can be derived from comparing LET measurements to those of other instruments (both on STEREO and other spacecraft such as ACE and GOES). Such comparisons have been made for individual SEP events (both large and small) at different times during the STEREO mission. These can be found in the following papers:

Cohen, C. M. S., Mason, G. M., Mewaldt, R. A., et al. 2008, Particle Acceleration and Transport in the Heliosphere and Beyond: 7th Annual International Astrophysics Conference, AIP, 1039, 118

Cohen, C. M. S., Luhmann, J. G., Mewaldt, R. A., et al. 2017a, Proceedings of 35th ICRC Conference, PoS(ICRC2017)134, 1

Cohen, C. M. S., Mason, G. M., & Mewaldt, R. A. 2017b, Astrophysical Journal, 843, 132

Mewaldt, R. A., Cohen, C. M. S., Cummings, A. C., et al. 2008, Proceedings of the 30th International Cosmic Ray Conference, 1, 107

Mewaldt, R. A., Leske, R. A., Stone, E. C., et al. 2009, Astrophysical Journal Letters, 693, L11

Wiedenbeck, M. E., Mason, G. M., Gómez-Herrero, R., et al. 2010, Twelfth International Solar Wind Conference. AIP Conference Proceedings,1216, 621

Calibration and Validation

The pre-flight and in-flight calibration of the STEREO LET instrument is described in detail in Section 4 of the LET instrument paper published in Space Science Reviews (SSR): Space Sci Rev (2008) 136: 285–3 ( <https://doi.org/10.1007/s11214-007-9288-x> ).

Pre-flight calibrations included:

* Electronic Pulser Calibrations
* Accelerator End-to-end Tests and Calibrations
* Radioactive Source Tests

The instrument was also calibrated in-flight early in the mission using in-flight particles. The stability of the detectors and electronics are monitored by checking whether the elements identified on-board remain centered in the bands in the three matrices as a function of time, temperature, and radiation dose (see Appendix D, Section 2.4). If not, it is possible to upload revised particle identification matrices, and this was done several times early in the mission. Large SEP events provide excellent statistical accuracy over a short time interval. Since the LET response overlaps with those of all three other SEP sensors, comparisons of the count rates, composition, and energy spectra between the four sensors make it possible to continually intercalibrate the SEP suite.

References

Mewaldt, R.A. et al, 2008, LET Instrument Paper: Space Science Reviews 136: 285–362 ( <https://doi.org/10.1007/s11214-007-9288-x> ).

Cohen, C. M. S., Mason, G. M., Mewaldt, R. A., et al. 2008, Particle Acceleration and Transport in the Heliosphere and Beyond: 7th Annual International Astrophysics Conference, AIP, 1039, 118

Cohen, C. M. S., Luhmann, J. G., Mewaldt, R. A., et al. 2017a, Proceedings of 35th ICRC Conference, PoS(ICRC2017)134, 1

Cohen, C. M. S., Mason, G. M., & Mewaldt, R. A. 2017b, Astrophysical Journal, 843, 132

Mewaldt, R. A., Cohen, C. M. S., Cummings, A. C., et al. 2008, Proceedings of the 30th International Cosmic Ray Conference, 1, 107

Mewaldt, R. A., Leske, R. A., Stone, E. C., et al. 2009, Astrophysical Journal Letters, 693, L11

Wiedenbeck, M. E., Mason, G. M., Gómez-Herrero, R., et al. 2010, Twelfth International Solar Wind Conference. AIP Conference Proceedings,1216, 621

Mewaldt et al, 2015, “A 360° survey of solar energetic particle events and one extreme event”. Proceedings of 704 Science. PoS(ICRC2015)139. 34th International Cosmic Ray Conference, The Hague. (2015)

Rodriguiz, J.V. et al, 2017, “Validation of the Effect of Cross-Calibrated GOES Solar Proton Effective Energies on Derived Integral Fluxes by Comparison with STEREO Observations, J. V. Rodriguez, Space Weather

###### Dynamic Thresholds

During large SEP events the single-detector count rates can increase by a factor of as much as 104 due mostly to low-energy protons. These elevated single-detector count rates create instrument dead-time and also lead to chance coincidence events involving two separate particles. In order to minimize these effects the LET design includes “dynamic thresholds” in which the trigger threshold on selected PHAs are increased during periods when the count rates are high. This action reduces the count rates of selected detectors, minimizing dead-time and effectively reducing the geometry factor for H and He events with minimal effect on the geometry factor for heavy ions with Z ≥ 6.


The dynamic thresholds are implemented in a 3-stage process that is controlled by the summed count rates of those selected detectors that do not participate, as summarized in Table 8 and Figure 3.6.3-1. In the first stage, the high-gain ADCs on all 20 of the L1 outer segments are disabled. The effective threshold for triggering these devices is thereby raised from ~0.25 MeV to the low-gain thresholds, nominally set at 5 MeV (see Table 7). The result is that neither H nor He ions can trigger these higher thresholds except for particles incident at very wide angles (see Figure 3.6.3-2). As a result, the geometry factor for H and He is reduced by a factor of 5.


In the second stage the high-gain ADCs are disabled on all but the center L1s (L1A2 and L1B2), providing a decrease in the effective geometry factor for H and He by a second factor of ~5. At this point LET has reduced angular coverage for H and He (~90° coverage instead of ~130°), but the angular coverage for Z ≥ 6 ions is not affected (except at the lowest and highest energies, where the L1 and L2 thresholds have some minor effects).

In the third stage the high-gain thresholds are disabled on all but the center two L2 segments on both the A and B sides (L2A4, L2A5, L2B4, L2B5 remain enabled), as well as the outside L3A and L3B segments. The nominal L2 and L3 low-gain thresholds are ~7 MeV and ~18 MeV, respectively, in order to be above the maximum energy loss of all but very wide-angle protons (see Figure 3.6.3-3). This effectively reduces the geometry factor for H and He by an additional factor of ~4.5.

The monitor count rate for this process is the sum of all singles rates that are not affected by these changes (the centers of L1A2 and L1B2; L2A4, L2A5, L2B4, and L2B5; and the centers of L3A and L3B). These monitor-rate trigger levels may be changed by command; the nominal levels are summarized in Table 8. In order to avoid toggling back and forth when the rates are near the trigger levels the dynamic thresholds for a given stage do not return to their nominal level until the count rates drop below the trigger level by some (commandable) factor (nominally = 2; see Table 8). By disabling the high-gain thresholds the singles rates in a large event like those of 14 July 2000 (Bastille Day event) and 28 October 2003 will be reduced by a factor of ~10, with a corresponding increase in livetime (see Figure 3.6.3-1). The state of the dynamic threshold currently implemented is indicated by two of the "miscellaneous bits" (see Table 20, Appendix 3) in the LET Science Data Frame, allowing the variable thresholds to be properly accounted for in calculating the true particle rates.

|  |  |  |  |
| --- | --- | --- | --- |
| Table 8: Dynamic Threshold Trigger Levels and Geometry Factors | | | |
| Affected Detectors | Trigger Rate  (counts/s) | Turn-Off Rate (counts/s) | H and He Geometry Factor (cm2sr) |
| L1 outsides | 1000 | 500 | 0.807 |
| L1 centers except L1A2 and L1B2 | 5000 | 2500 | 0.175 |
| All L2s but L2A4, L2A5, L2B4, L2B5; L3 outsides | 25,000 | 12,500 | 0.039 |

**Fig. 27** Illustration of the effect of dynamic thresholds on the count rates and event readout from LET during a solar event with the composition and spectra of the July 14, 2000 (Bastille Day), SEP event. As the thresholds of various detector segments are gradually raised in response to the Monitor rate, the measured singles rate (labeled “scaled Singles”) and the H and He event rates are reduced, thereby preserving instrument livetime to record a greater sample of *Z* ≥ 6 events

**Fig. 28** Illustration of the nominal and dynamic thresholds for L1A•L2A events (*left panel*) and for L1A•L2A•L3A events (*right panel*)

###### Release Notes and Caveats

Cumulative Release Notes for LET Level 1 data - Public data set.

See http://www.srl.caltech.edu/STEREO/docs/LET\_Level1.html

for more LET Level 1 data documentation.

April 3, 2013: Important Update: Due to incorrect calculation of instrument

livetimes in ground data processing, LET intensities at the peak of the July

23 2012 event were inaccurate. LET intensities during other periods of high

particle intensities were also inaccurate to a lesser extent. We have

corrected the livetime calculation, and a new version of the data has been

released - Version 11.

Dec 3, 2012: Important Update: Due to incorrect calculation of instrument

livetimes in ground data processing, LET intensities at the peak of the July

23 2012 event are inaccurate. We are working on a correction to the livetime

calculation, and expect to reprocess these data soon.

April 16, 2012

The 15-21 MeV/nuc Carbon bin is not valid during high-rate periods

(periods when the LET dynamic-threshold stats is >0). It is therefore set to

"Fill data" for these periods.

The instrument thresholds are higher during these periods, and particles in

this species-energy bin fall below the raised thresholds in some cases.

April 16, 2012

The total-energy calculation for particles that penetrate the instrument

to Range 4 was found to be implemented incorrectly. The LET instruments on

Ahead and Behind have been patched to correct the error.

LET Ahead was patched on April 16, 2012.

LET Behind was patched on April 18, 2012.

Prior to these dates, the following species-energy bands are invalid.

The LET data prior to the above patch dates are now reprocessed to replace

the data in these bins with "FILL data".

H: 12 - 15 \*

4He: 12 - 15

C: 21 - 27 \*

C: 27 - 33 \*

N: 21 - 27

N: 27 - 33 \*

O: 27 - 33 \*

Ne: 27 - 33 \*

Ne: 33 - 40 \*

Mg: 33 - 40 \*

Mg: 40 - 52 \*

Si: 33 - 40

Si: 40 - 52 \*

Fe: 40 - 52

Fe: 52 - 70 \*

Note: the species-energy bands marked with "\*" above were already suppressed in the

Public data, for other reasons. So, this issue actually affects only 4 bands.

October 14, 2011

The LET instruments on Ahead and Behind have been patched to correct the

instrument response when the instrument is in its "dynamic thresholds" mode

during high rate periods.

LET Behind was patched on October 11, 2011

LET Ahead was patched on October 14, 2011.

After these dates, the energy-bands for "heavies" that were invalid during high-rate periods

are now usable and are no longer being excluded from public release.

September 8, 2011

Due to unexpected changes in the LET instrument response when the instrument is in its

"dynamic thresholds" mode during high rate periods, we have replaced with "FILL data" the

data a subset of the energy-bands for for C, N, O, Ne, Na, Mg, AL, and Si, during high-rate

periods (approximately when 1.8-3.6 MeV proton intensities exceed ~150 counts/(cm^2 sr s MeV)).

We expect to upload a flight-software fix for this issue soon.

See Nov 11, 2010 note for more details of the issue.

November 22, 2010

We made some changes to the species represented in the LET sectored rates.

After Nov 22, 2010, the sectored rates are assigned as follows:

0 - 15: H 4-6 MeV/nuc

15 - 31: H 1.8-3.6

32 - 47: 4He 4-6

48 - 63: 4He 6-12

64 - 79: CNO 4-6

80 - 95: CNO 6-12

96 - 111: NeMgSi 4-6

112 - 127: NeMgSi 6-12

128 - 143: Fe 4-12

144 - 159: H 6-10

Prior to Nov 22, the rates were:

0 - 15: H 4-6 MeV/nuc

15 - 31: 3He 4-6

32 - 47: 4He 4-6

48 - 63: 4He 6-12

64 - 79: CNO 4-6

80 - 95: CNO 6-12

96 - 111: NeMgSi 4-6

112 - 127: NeMgSi 6-12

128 - 143: Fe 4-6

144 - 159: Fe 6-12

November 11, 2010

Recently we have discovered some unexpected changes in the LET instrument

response when the instrument is in its "dynamic thresholds" mode during

high rate periods. During such periods, calibration shifts have been found

that cause some counts for some elements to be mislabeled as the

neighboring elements. At present, only ~4-10 MeV/nuc C, N, O, and Ne on the

Behind spacecraft have been affected, and only during two time intervals

during the SEP events of 2-3 August 2010 (day of year 214 and 215). Rates

for these elements are inaccurate by perhaps as much as a factor of ~2

from approximately 6:41 through 14:44 on day 214 and again from 4:29

through 9:07 on day 215 of 2010. Until we can develop and implement

commands to fix the problem (which we are working on), these errors will

also recur during any similar high rate periods (approximately when 1.8-3.6

MeV proton intensities exceed ~150 counts/(cm^2 sr s MeV)) on both

spacecraft in the future. Note that this problem does NOT affect the

data during the large SEP events of December 2006 since the instruments

were in a different mode at that time.

March 20, 2008

The geometry factors used to calculate intensities are under review.

A new version of the LET Level 1 data will be released at some point in the future, using new geometry factors. The resulting changes from the current version will be on the order of 5%, or less.

Sept 4 2007

LET Level 1 software version 09.

Updated sectored geometry factors.

July 31, 2007

LET Level 1 software version 08.

First public data release.

See http://www.srl.caltech.edu/STEREO/docs/LET\_Level1.html for more

LET Level 1 documentation.

For the Public data set, we are currently flagging as bad

the He data prior to March 29 2007, and the 3He data after March

29 2007. In addition, the following species/energy-bin channels are

also flagged as bad in Public data set:

All Protons prior to the March 29 software uploads.

Protons below 4 MeV after the March 29 software uploads.

All 3He, for all time periods.

All 4He prior to the March 29 software uploads.

Fe below 5 MeV prior to the March 29 software uploads.

Fe below 4 MeV after the March 29 software uploads.

One or two energy-bins at the low and/or high ends for

many species.

June 21 2007

LET Level 1 software version 08.

Added sectored data files.

June 14 2007

LET Level 1 software version 08.

This version includes the following changes from the previous version:

Added, Na, Al, S, Ar, Ca, Ni to output data files.

Added elemental helium.

After March 29, 2007, (at slightly different times on each spacecraft)

events identified as 3He onboard are treated like 4He for

energy-binning (a mass-number equal to 4 is used). This allows the 3He

and 4He boxes to be combined on the ground to obtain elemental helium

(He) intensities. For data prior to the March 29 software uploads,

the He data are FILL (-9999.9).

For data after the March 29 software uploads, the 3He data are FILL.

Improved software for reading in time-dependent factors files, and

created new factors files for some time periods in Nov and Dec 2006

when the instruments were in funny states.

Added capability to flag each species/energy-bin channel as either

"good" or "bad" for any time period. Bad channels are set to FILL.

The flags for different time periods are stored as external tables,

and the tables are read as needed depending on the time-stamp of the

data being processed.

/home/stereo/LETL1Data/SRLonly/

Factors\_files/

ReleaseNotes.txt

ahead/

2006/

1Minute/

Sectored/ (contains 1Minute-averaged ahead sectored daily files for 2006)

Standard/ (contains 1Minute ahead unsectored daily files for 2006)

Summed/ (contains 1Minute ahead summed energy-bin daily files for 2006)

10Minute/

Sectored/ (contains 10Minute-averaged ahead sectored files for 2006, with a month of data in each file)

Standard/ (contains 10Minute-averaged ahead unsectored files for 2006, with a month of data in each file)

Summed/ (contains 10Minute-averaged ahead summed files for 2006, with a year of month in each file)

Hourly/

Sectored/ (contains Hourly-averaged ahead sectored files for 2006, with a year of data in each file)

Standard/ (contains Hourly-averaged ahead unsectored files for 2006, with a year of data in each file)

Summed/ (contains Hourly-averaged ahead summed files for 2006, with a year of data in each file)

Daily/

Sectored/ (contains Daily-averaged ahead sectored files for 2006, with a year of data in each file)

Standard/ (contains Daily-averaged ahead unsectored files for 2006, with a year of data in each file)

Summed/ (contains Daily-averaged ahead summed files for 2006, with a year of data in each file)

2007/ and so on...

behind/

Same organization as for ahead

###### Pointing and Orbit Data for the SEP Instruments on the STEREO Spacecraft

This document provides information about orientation of the LET instrument on the STEREO Ahead and Behind spacecraft, and instructions for calculating pointing (attitude) and position vectors for any SEP instrument from the spacecraft ancillary data.

* Sections 1 and 2 deal with defining a LET coordinate system, and provide a recipe for converting vectors in the LET system to the spacecraft coordinate system. No recipe is provided for the other SEP instruments – this is left to the respective instrument teams.
* Section 3 describes a procedure for transforming pointing vectors in the spacecraft coordinate system to other useful coordinate systems, using transformation matrices provided by Caltech. These transformation matrices are provided in text data files, and the format of these files is described.
* Section 4 describes the format of the STEREO orbit data text files provided by Caltech.

# LET Orientation with Respect to the Spacecraft Coordinate System

## Both Spacecraft

For both spacecraft:

* LET is mounted on the S/C +Y panel.
* The S/C +X axis points sunward.
* During normal flight operations, the S/C X-Z plane and the ecliptic plane will generally be co-planar, approximately.

For both spacecraft, we define a LET coordinate system as follows:

* X: center of LET forward Field of View (FOV).
* Y: outward from spacecraft (same as S/C +Y axis).
* Z: completes the right-hand orthogonal set.

For the purposes of this discussion, we may ignore the fact that the origins of the LET and S/C origins are not co-located.

## Ahead Spacecraft

The Ahead S/C Y-axis points towards the north ecliptic pole. The LET X-Z plane is rotated θ = +45° about the S/C Y-axis (see Figure 1). To transform a vector **v** in the LETa system to a vector **v′** in the S/Ca system,

**v′ = Ta** **v**

where **Ta** = 




Figure 1: LET mounting and orientation on the Ahead Spacecraft, showing S/C X, Y, and Z axes. For illustration purposes only, positions and dimensions not exact.

## Behind Spacecraft

The Behind S/C Y-axis points towards the south ecliptic pole. A diagram of the LET mounting on the Behind spacecraft is TBD. The LET is mounted in a different position on the S/C +Y panel, and the LET X-Z plane is rotated θ = -45° about the S/C Y-axis (note the negative angle). The transformation matrix to transform a vector **v** in the LETb system to a vector **v′** in the S/Cb system is the same as for the Ahead S/C: just be sure to use the correct sign for the angle θ.

# LET Sectors (Look Directions)

The various combinations of L1 and L2 segments define a total of 300 different directions in the LET X-Z plane. These directions are sorted during onboard data processing into sixteen sectors, defined in Table 1.

Table 1: LET Detector Combinations Sorted into Sectors



Each sector points in a direction defined by an angle with the LET +X axis. From this angle, the pointing vector for each sector may be calculated. The angles and pointing vectors (in the LET and the S/C coordinate systems) are listed in Table 2.

Table 2: LET Sector Pointing Vectors, in the LET and S/C coordinate systems.



Note: The **y** component of all LET pointing vectors is zero, in both the LET and S/C coordinate systems.

Figure 2 below shows the coverage in longitudinal angle for each of the LET sectors.

The "Longitude from LET Axis" is the same angular measure as in column 3 of Table 2 above. Basically, the view cones are ~± 8 deg in the ecliptic and ~ ± 14° out of the ecliptic, except for the outside segments which are twice as wide. There are some variations from center to edge.




Figure 2: Coverage in longitudinal angle for each of the LET sectors.

# Transformations from Spacecraft to Other Coordinate Systems

We have described the transformation of vectors from the LET to the S/C coordinate system. This section summarizes the procedures for transforming vectors in the S/C coordinate system to other useful coordinate systems.

The STEREO Science Center provides IDL SPICE software via the Solarsoft library that facilitates the transformation of vectors in the S/C coordinate system to other useful coordinate systems. The full list of supported coordinate systems and their descriptions may be found in the STEREO Solarsoft documentation. The subset currently assumed to be useful for LET data analysis is listed and described in Appendix B (more can be added as needed). The descriptions are copied from the STEREO Solarsoft documentation. Included are GEI, GSE, GSM, RTN, and several heliocentric coordinate systems.

**Since a number of SEP team investigators either do not use IDL, or do not wish to install Solarsoft, Caltech provides text files containing transformation matrices for converting vectors from the S/C coordinate system to the coordinate systems listed in Appendix B. The format of each record in these files is as follows:**

YYYY DoY Second Flag M\_00 M\_01 M\_02 M\_10 M\_11 M\_12 M\_20 M\_21 M\_22

Where YYYY is the 4-digit year

DoY is the day-of-year (counting from 1)

Second is the second-of-day

Flag is 0 if the data are predictive

1 if the data are definitive

M\_ij are the transformation matrix elements from the S/C coordinate system to the new coordinate system, where i is the row index, j is the column index.

The time cadence of records within these files is variable. A new record is appended only

* at the beginning of each day, **or**
* if the direction of the S/C X-axis changes by more than TOL degrees, **or**
* if the direction of the S/C Y-axis changes by more than TOL degrees

TOL is currently set to 0.25 degrees.

# STEREO Orbit Data

The STEREO Science Center provides IDL SPICE software via the Solarsoft library that returns the coordinates of either of the two STEREO spacecraft in any of the supported coordinate systems. **Again, since a number of SEP team investigators either do not use IDL, or do not wish to install Solarsoft, Caltech provides text files containing position coordinates for the ahead and behind spacecraft in the coordinate systems listed in Appendix B (except for HGRTN/RTN) . The format of each record in these files is:**

YYYY DoY Second Flag P\_0 P\_1 P\_2

Where YYYY is the 4-digit year

DoY is the day-of-year (counting from 1)

Second is the second-of-day

Flag is 0 if the data are predictive

1 if the data are definitive

P\_i are the components of the spacecraft position vector in the given coordinate system.

The time cadence of records within these files is variable. A new record is appended only

* at the beginning of each day, **or**
* if the position of the S/C changes by more than TOL kilometers from the previous position.

TOL is currently set to 1000 km.

Transformation matrices for converting vectors from the S/C coordinate system to these coordinate systems are provided by Caltech as text files to the SEP instrument teams.

# Coordinate Systems useful for LET Data Analysis

**GEI: Geocentric Equatorial Inertial**. The *X* axis points toward the first point of Aries (i.e. the vernal equinox), and the *Z* axis is aligned with the geographic north pole. When expressed in terms of longitude and latitude, this is the well known celestial coordinate system of right ascension and declination. This is realized with the J2000 ecliptic.

**GSE: Geocentric Solar Ecliptic**. *X* is the Earth-Sun line, and *Z* is aligned with the north pole for the ecliptic of date.

**GSM: Geocentric Solar Magnetospheric**. *X* is the Earth-Sun line, and *Z* is the projection of the north dipole axis.

H**CI: Heliocentric Inertial**. *Z* is the solar north rotational axis, and X is the solar ascending node on the J2000 ecliptic.

**HEE: Heliocentric Earth Ecliptic**. *X* is the Sun-Earth line, and *Z* is the north pole for the ecliptic of date.

**HEEQ: Heliocentric Earth Equatorial**. *Z* is the solar rotation axis, and *X* is in the plane containing the *Z* axis and Earth, at the intersection of the solar central meridian, and the heliographic equator. When converted to longitude and latitude, this is known as Stonyhurst heliographic coordinates. In FITS files, this coordinate system is abbreviated as “HEQ”, so that variation is also recognized by the software.

**HGRTN/RTN: Radial-Tangential-Normal**. *X* axis points from Sun center to the spacecraft, and the *Y* axis is the cross product of the solar rotational axis and *X*, and lies in the solar equatorial plane (towards the West limb). For the STEREO Ahead spacecraft, this is realized through the dynamic coordinate frame STAHGRTN, while for STEREO Behind it is realized through STBHGRTN. When the Sun is used as the origin, the designation is HGRTN—with the spacecraft as origin, it’s simply RTN.

###### LET Telemetry Data Format

The science data telemetry format document is included below as a reference (starting next page),

1. **LET Science Data Frame Format**

Allan Labrador (labrador@srl.caltech.edu), Caltech

9 April 2007 (Version 13.0)

(Slightly modified 8/30/07)

**1.0 Introduction**

The purpose of this document is to describe the science data that will be transferred from the LET MISC to the SEP Central MISC. The format does not describe beacon data, nor does it describe CCSDS packet header or checksum information.

This document makes reference to information in the following external documents:

* LET Science Requirements Document
* *STEREO SEP LET and SEP Central: Flight Software Requirements* (*Version F, STEREO-CIT-002.F*)
* *STEREO IMPACT SEP Sensor Suite Commanding and Users Manual* (*Version F, STEREO-CIT-007.F*)
* *Specification of Functional Test Modules and In-flight Calibration Routines for LET* (*STEREO-CIT-006.A*)
* *STEREO/IMPACT LET Detector Naming* (*STEREO-CIT-0015.B*).
* *LET Software Counter Definitions* (*STEREO-CIT-019.A*).
* Interface Control Document (ICD) for the IMPACT Investigation.
* CCSDS 102.0-B-5 Packet Telemetry, Blue Book, Issue 5

Information is also included from other documents, memos, e-mail messages, discussion not in the formal STEREO/IMPACT document collection. Elements to be resolved or to be determined, or elements documented only in software, are marked **TBD.**

In this document, “LET Science Frame” and “LET Science Data Frame” may be used interchangeably.

**2.0 LET Science Data Frame Format -- Requirements and Goals**

The LET Science Data Frame Format is designed to accommodate the following LET Science requirements and goals, abstracted from the LET Science Requirements Document:

Table 1.1: Selected LET Science Requirements and Goals

|  |  |  |
| --- | --- | --- |
|  | **Requirements** | **Goals** |
| **Event (Pulse Height) Telemetry Rate** | 1 event/sec with prioritization | ~4 events/sec with prioritization |
| **Species Coverage (rates data)** | 10 species (H, 3He, 4He, C, N, O, Ne, Mg, Si, Fe) | 16 species (H, 3He, 4He, C, N, O, Ne, Na, Mg, Al, Si, S, Ar, Ca, Fe, Ni) |
| **Energy bins (rates data)** | 3 intervals for H  6 intervals for Z≥2 | multiple energy bins, depending on species and penetration range |
| **Event processing rate (rates data)** | 1000 events/sec | ~5000 events/sec |
| **Telemetry interval (time resolution) for rates data** | 15 minutes for all species | 1 minute for all species |

The LET Science Data Frame Format as described in this document will attempt to accommodate the rates-related Goals listed in Table 1.1.

The LET Science Data Frame Format is also designed with the following software engineering goals as guidance:

* Maximize bandwidth usage (i.e. minimize number of unused bits)
* Maximize event data (pulse height) bandwidth allocation
* Align data elements to nibble (4-bit) boundaries, byte boundaries, or MISC word (24-bit) boundaries, to simplify data examination in hexadecimal format
* Send data at short, regular intervals to the SEP Central MISC, to allow for faster debugging.
* In the event of bit errors (expected to be extremely rare), event data should be as reconstructible as possible to reduce the fraction of corrupted event data.

LET is allocated 16 CCSDS packets per minute, out of the 36 CCSDS packets per minute allocated to SEP. The 11 byte header and 1 byte checksum for each 272 byte CCSDS packet are not included in the LET Science Data Frame Format. Therefore, one minute of LET Science Data corresponds to 16\*260 = 4160 bytes. Define these 16 CCSDS packets (minus headers and checksums) as one LET Science Data Frame, for transmission from LET to the SEP Central MISC. The goal is to accumulate and transmit all science rates (species counts) in one minute intervals, so that each LET Science Data Frame contains a complete set of science rates for a given minute.

According to the *SEP LET and Central MISC Processors Flight Software Requirements* document (Version E), the LET MISC will have opportunities to transmit complete CCSDS packets (with headers and checksum) to the SEP Central MISC once every three seconds. It is left to the SEP Central MISC to fill in time stamps and checksums in the CCSDS packets before passing them to the IDPU. The LET MISC will fill in ApIDs and source sequence counters and other pack identification information. A complete LET Science Frame is transmitted each minute, with rates and pulse heights having been packed into the Science Frame format and divided into CCSDS packets during the previous minute. If the event buffer (Section 2.8) does not get filled to the point of requiring the full 4160 byte allocation of the LET Science Frame, the LET MISC will fill the remaining packets with 0’s.

The flow of data from LET to the IDPU is represented graphically in Figure 1.1.






Figure 1.1: Data flow from LET to IDPU



(a)



(b)

Figure 1.2: LET Science Frame Overview, (a) without CCSDS packet headers and checksums, and (b) with CCSDS packet headers and checksums. LET Science Frame Header is unlabeled at upper left. (Data elements not to horizontal scale.)

A LET Science Frame is shown graphically in Figure 1.2, with and without CCSDS packet headers and checksums. It includes 16 CCSDS packets for a total of 4160 bytes (not including CCSDS packet headers and checksums). Rates data occupy ~5.5 CCSDS packets. Event data occupy the remaining CCSDS packets.

Note that, although LET will be transmitting one science data packet every three seconds, only the first 16 of those packets will comprise a science frame. Within the science frame, unused event buffer space will be filled with 0’s. The spare frames will also be filled with 0’s and assigned a unique ApID.

**2.1 Byte Order**

The LET Science Frame is envisioned as an array of bytes or as a stream of bytes. Transmission of data elements is also envisioned as a stream of bytes. When a LET Science Frame element spans more than one byte, it will be transmitted high-byte-first. For example, Event Buffer Headers (Section 2.8) span four bytes, or one MISC word plus one byte, and these will be transmitted in the order of highest byte, second high byte, second low byte, and lowest byte.

**2.2 ApID and Packet Number**

The ApID value of 580 is assigned to every LET Science Frame Packet, and this value is stored in the CCSDS packet header (not part of the LET Science Frame itself). In order to identify individual packets within the LET Science Frame, bits 0–3 of the subseconds field of the CCSDS packet header are replaced by a packet number. The packet numbers are defined in Table 2.1, as also shown in Figure 1.2.

Table 2.1: LET Science Packet Numbers

|  |  |
| --- | --- |
| **Packet #** | **Packet Description** |
| 0–4 | Science Frame Header, Counters and Rates |
| 5 | Counters and Rates, start of Event Buffer |
| 6-15 | Event Buffer frames |

The ApID and packet numbers will be assigned by the LET MISC and entered into each CCSDS packet header. The LET Science Data Frame does not make direct use of the source sequence counter in each CCSDS packet header.

**2.3 LET Science Frame Header**

Some header information is included in the CCSDS packet headers (secondary headers). However, because CCSDS packet formatting may be removed during ground-based analysis in order to extract full LET Science data from each set of LET CCSDS packets, it will be useful to include a LET Science Frame Header.

The LET Science Frame Header is allocated as 5 bytes at the top of the LET Science Frame. Byte 0 is the spacecraft ID (SCID) and frame version number (SFVER). The two most significant bits are the spacecraft ID — 00 for the EM unit (no spacecraft), 01 for FM1 (the leading spacecraft, or "ahead"), and 10 for FM2 (the trailing spacecraft, or "behind"). The remaning bits are a LET Science Frame Version number; the current version number is 11. Should the version number ever exceed 128, the version number in these bits will be calculated modulo 128.

Bytes 1 and 2 (high byte and low byte – see Section 2.1) contain the number of valid bytes (SFLEN) in the complete LET Science Frame (not including CCSDS header and checksum). “Valid” bytes include all the bytes from the frame header to the last byte of the last event in the event buffer, and this counter does not include CCSDS packet headers or checksums. Because 6 CCSDS packets containing fixed format data are always present, this number is never less than 1418. This number never exceeds 4160. The three most significant bits of byte 1 are unused.

The last two bytes (bytes 3-4) of the LET Science Frame Header are defined as a checksum (SFCHECK, to verify the integrity of the LET Science Frame Data. The checksum algorithm is **TBD**. It is proposed that the two bytes be set such that the sum of all bytes or MISC words modulo 216 equal zero. Individual bytes are summed, with the checksum allowed to grow to 16 bits. This checksum is independent of the CCSDS packet checksums and is calculated by the LET MISC prior to the calculation of CCSDS packet checksums by SEP Central.

The contents of the LET Science Frame Header are summarized in Section 3.0.

**2.4 Science rates (species counts, rate counters):**

For the science rates coming with each frame, counts for H and He (He-3 and He-4), 13 heavy elements (C, N, O, Ne, Na, Mg, Al, Si, S, Ar, Ca, Fe, and Ni), and various “background” counts (including charge ranges) will be transmitted. Science Rates will be organized top–down in order of penetration range, then species, then energy. Science rates included in the LET Science Frame are summarized in Tables 3.9–3.14, and their locations in the LET Science Frame are detailed in the same tables.

As described in the *STEREO SEP LET and SEP Central Flight Software Requirements (Version F, STEREO–CIT–002.F)* document, particles which pass certain onboard processing cuts are sorted into matrices according to their penetration range in the instrument and by delta–E vs. E’ measurements. Each matrix represents a penetration range — into the L2 detectors (RNG2, or L1L2), into one L3 detector (RNG3, or L2L3), or into two L3 detectors and possibly beyond (RNG4, PEN, or L3AL3B). Within each penetration range, the associated matrix covers a delta–E vs. E’ space that spans particles from Z=1 (H) to Z≥40 (Zr). The matrices are used by onboard processing to identify particles by range in the instrument and charge, and further onboard processing is used to determine particle kinetic energy. The matrices span 128 bins in the x–axis and 400 bins in the y–axis, and they are shown graphically in Appendix C. (Note that this LET Matrix information supercedes details in *STEREO–CIT–002.F, Appendix 1*, which is out of date as of this version of the LET Science Data Format.)

Particles that are sorted through the matrices are counted in arrays in the LET onboard memory, sorted by penetration range, species (element, charge, charge range, or background), and energy (for elements). Particle counting rates with defined element and energy are termed “foreground rates” (FGRATES), following the curved tracks bounding elements in the Figures in Appendix C. Foreground rates include elements (and helium isotopes) such as H, He-3, He-4, C, N, O, Ne, Na, Mg, Al, Si, Ar, Ca, Fe, and Ni. Particles counted by the FGRATES are assigned Particle IDs which equal their index values in the FGRATES arrays associated with each penetration range (L1L2=L2FGRATES, L2L3=L3FGRATES, L3AL3B=PENFGRATES). These Particle IDs are also used to identify particles in the Event Record Headers, described in Section 2.8. The Particle IDs are given in Tables 3.9–3.14. Particles not located in the FGRATES regions of the matrices, or particles which are otherwise unclassified by the matrices, are assigned a Particle ID of 255. Note that some elements are classified by the Range 3 matrix but not in the other matrices. These particles are also assigned a Particle ID of 255 when located in the Range 2 or Range 4 matrices, e.g. Na in RNG 2 and RNG 4.

Particle IDs may be duplicated between different ranges. While it may be convenient for science analysis for particles having the same charge and energy range in two different matrices to have the same Particle ID, it would add additional load to limited onboard computing resources. It will be less strain on computing resources to account for different Particle IDs during analysis on the ground.

Particles in the matrices which do not fall along element or isotope tracks are termed “background rates” (BGRATES). Background rates are counts from broad regions of delta–E vs E’ space in the matrices such as the Li, Be, and B region between He and C, or the “backward moving particles” region to the lower right corner of delta–E vs. E’ plots. The background rates also include regions covering STIM events, described elsewhere. All background rate events are assigned Particle ID 255. The background rates are summarized in Tables 3.9–3.14.

Finally, science rate counters are stored in onboard memory in 24 bit counters, but in the Science Frame, these rates are compressed to 16 bits. The format for the compressed, 16 bit rates is shown in Figure 2.1.




Figure 2.1: 16 bit compressed rate.

The compression algorithm will be a 16 bit modified biased exponent hidden one algorithm, as detailed in Appendix A.

Thus, there are currently 371 Science Rates in the LET Science Data Frame, for a total of 742 bytes.

**2.5 Look Direction Rates**

Under the current LET Science Frame Format, 8 look directions toward the A side of the LET detector and 8 look directions toward the B side of LET will be counted, for 10 rates in each direction. A total of 160 look direction rates will be encoded in the LET Science Frame. Each look direction rate will be encoded in 16 bit compressed rates, using the same format and compression/decompression algorithm as the science rates. Thus, we send a total of 320 bytes of look direction rates per LET Science Frame.

The look directions are divided into 8 sectors on either side of LET, with detector combinations currently described elsewhere. (See *Options for LET Sectored Rates* and *Final Selection of Sectored Rates (9/29/03)* memos (R.A. Mewaldt).*)* For the purpose of the LET Science Frame Format, the 8 sectors are numbered 0 through 7, and they are geometrically arranged clockwise around the LET detector, so that sector 0 of LET side A is associated with the L1A0 detector, and sector 7 of LET side A is associated with the L1A4 detector. (See *STEREO/IMPACT LET Detector Naming, STEREO-CIT-0015.B.*) Numbering on the B side begins with direction 8, so that sector 8 of LET side B is associated with the L1B0 detector, and so on.

In addition to look directions, or sectors, these rates are divided into element or element ranges: H, He–3, He-4, CNO, NeMgSi, and Fe. Within each element, these rates are further divided into energy ranges.

Organization of the look direction rates arranged top–down by species, energy range, and look direction, with look direction first on side A (directions 0 through 7) and then side B (directions 8 through 15). The look direction rates are summarized in Section 3, Table 3.15:

**2.6 Singles and Coincidence Rates**

There are 54 ADCs in LET, and each ADC will be measured for singles rates at low and high gain thresholds. These rates will be compressed to 16 bits, using the same compression/decompression algorithm employed for science and look direction rates. Thus, there will be a total of 108 singles rates in the LET Science Frame, for a total of 216 bytes. The singles rates are given in order of detector address number, which is used by the LET onboard software for detector addressing. The ordering of singles rates in the LET Science Format is top–down by detector number, then by high gain and low gain. Thus, the first four bytes in the Singles Rates block are L2A0 (detector address 0), with the first two bytes being L2A0 high gain singles rate, and the second two bytes being L2A0 low gain singles rate. (Furthermore, given the byte ordering described in Section 2.1, the first byte of the L2A0 high gain singles rate is the high byte, and the second byte is the low byte.) See Section 3, Table 3.4 for a summary of the singles rates and their location in the LET Science Frame, and see the *LET Detector Naming* Document for a description of the detector naming convention.

Coincidence rates are listed in Section 3, Table 3.7. These rates count coincident hits for detector groups for the minute spanned by the Science Frame. Space in the LET Science Frame is allocated for 12 coincidence rates (including 2 unused spares), compressed to 16 bits as with other rates.

**2.7 Livetimes, Event Processing Counters, and Priority Buffer Counters**

Space is allocated in the LET Science Frame for livetime counters, event processing counters, and priority buffer counters. These counters are event or processing counts used or otherwise maintained by the LET onboard software, and they are partially described in *LET Software Counter Definitions* (*STEREO-CIT-019.A*) and in no other formal STEREO/LET Documents. These counters should be formally described in the LET Documentation — **TBD**. The use of the livetimes to calculate intensities should also be formally described.

LET Livetimes, event processing counters, and priority buffer counters are listed in Section 3, Tables 3.3, 3.6, and 3.8, respectively. All of the counters are stored as 24 bit numbers in the LET onboard memory, and in the LET Science Format, they are compressed to 16 bits using the same compression algorithm as is used with the science rates. The one exception is the Front End Electronics livetime counter (bytes 8–7 in the LET Science Frame), which is scaled from 24 bits to 16 bits.

Notes on Table 3.3: The NUMTRIG, NUMREJECT, etc. counters are hardware counters, with counters for events taken under hazard (.HAZ) conditions. NUMTRIG is the number of trigger events detected by the hardware during every even numbered second during the minute of accumulation time for the science frame. NUMREJECT is the number of trigger events rejected for further analysis, as determined by hardware conditions described elsewhere. NUMACCPHA is the number of trigger events accepted for further analysis with PHA data, as determined by the hardware. NUMACCNPHA is the number of trigger events accepted for further analysis without PHA data; however, since all accepted events currently include PHA data, this number is always zero. Under the current definitions, the sum of NUMREJECT and NUMACCPHA should equal NUMTRIG. Because these counters are accumulated only during even numbered seconds, they represent only half the total number of triggers, etc. which could be detected during the entire minute

The equivalent .HAZ counts are those counted under hazard conditions, and these are accumulated during odd numbered seconds during the minute. A trigger event is flagged as a .HAZ event if it comes within 18/6.4 (~2.8) microseconds after the previous trigger. The .HAZ condition is an added condition to the trigger logic; it is not exclusive. Therefore, if NUMTRIG and NUMTRIG.HAZ events were counted simultaneously, the NUMTRIG.HAZ events would count a subset of the NUMTRIG events. The NUMREJECT.HAZ and NUMACCPHA.HAZ events are defined as NUMREJECT and NUMACCPHA events, only with the .HAZ condition added. As with non-.HAZ events, the .HAZ events represent only half the total number of .HAZ events which could occur during a given minute, since they are accumulated only during odd numbered seconds.

Currently, all .HAZ events are rejected for analysis, though this rejection can be commanded on or off. The livetime counter is not incremented during .HAZ events, when such events are rejected for analysis.

**2.8 Miscellaneous Bits and Rates — TBD**

Some information regarding the state of the instrument and software, as well as rates not defined in previous sections, are allocated space in the LET Science Frame. Two bytes of MISCBITS and 10 bytes of MISCRATES are allocated to the LET Science Frame, and these bits and bytes are located in the Frame in Section 3, Tables 3.2 and 3.5. MISCBITS contain information via software flags on the state of the instrument and a minute counter; MISCRATES are currently **TBD**.

**2.9 Event Buffer – Event Record Format:**

With the fixed format data described in previous sections for the LET Science Frame, there remain 2733 bytes, all of which will be pulse height data in an Event Buffer. Events (pulse heights) are sampled by the LET MISC from priority buffers listed in Section 3, Table 3.8 and described in separate documentation (**TBD**), and the sampled pulse heights are packaged into Event Records in the Event Buffer. The telemetered events will not exceed the Event Buffer length.

At the top of the event buffer will be a header containing the number of events saved to the buffer. If the minimum event length of 2 ADC hits is 72 bits (9 bytes – see below), then the event buffer can contain up to ~303 events, with one 2 byte event buffer header. Unused buffer space will be filled with $00’s, and empty packets will not be transmitted.

Within the buffer, each event should be collected in a defined event record, composed of an Event Record Header (ERH) followed by a variable number of ADC fields. The 32 bit Event Record Header is defined as follows:

Table 2.2: Event Record Header (ERH)

|  |  |  |
| --- | --- | --- |
| **Data** | **Bit** | **Note** |
| **Particle ID** | 0–7 | = particle ID if the particles are sorted by the LET Matrices as “foreground” particles. (=255 if the particles are not sorted by the matrices or are identified as background particles). Allows matrices to ID particles by range (matrix), species, and energy. See Section 3, Tables 3.9–3.14 for lists of Particle IDs. See also *SEP LET and Central MISC Processors Flight Software Requirements* (*STEREO-CIT-CIT-002.F*). |
| **Priority Buffer Number** | 8–12 | See Section 3, Table 3.8 for a list of Priority Buffer Numbers and their descriptions. See also *LET Software Counter Definitions* (*STEREO-CIT-019.A*), and uncatalogued memos by RAM (**TBD**). |
| **L1A Tag** | 13 | Indicates an L1A detector contributed to the coincidence trigger |
| **L2A Tag** | 14 |  |
| **L3A Tag** | 15 |  |
| **L1B Tag** | 16 |  |
| **L2B Tag** | 17 |  |
| **L3B Tag** | 18 |  |
| **STIM Tag** | 19 | Flags a STIM event. |
| **HAZ Tag** | 20 | Hazard flag. |
| **Time Tag (Latency Bits)** | 21–24 | Duplicates the 4 least significant bits of the LET onboard minutes counter (Section 2.8, and Table 3.2); used to identify event latency |
| **A/B Event Tag** | 25 | A=0, B=1 |
| **# Unread ADCs** | 26–28 | # hit ADCs not include in the Event Record. Saturates at 7. |
| **Extended Header Flag** | 29 | =1 if an additional header byte (or set of bytes) is appended to this header (**TBD**) |
| **STIM Block Flag** | 30 | =1 if STIM Information Block is included in this event |
| **Culling Flag** | 31 | =1 if number of ADCs culled from this event is nonzero. |

The format of the event record header is summarized in Figure 2.2:




Figure 2.2: Event Record Header, 32 bits.

The particle ID identifies the particle by species and energy, based on how it was sorted through the LET Matrices (Section 3, Tables 3.9–3.14, and Appendix C). If the particle is not a “foreground” event (i.e. if it is not identified as a selected element or helium isotope for a given matrix) and is instead a “background” event, or if the particle is not sorted by the LET matrices, it is assigned a Particle ID of 255. For the identifiable elements targeted by the LET instrument (Table 1.1), the Particle ID is sufficient to identify element and energy.

Additional information is provided by the priority buffer number (bits 8–12). This number identifies the priority buffer from which the Event is taken. Although all events in the Event Buffer are taken from the Priority Buffers, not all events are sorted by the LET Matrices. Not all particles which trigger the LET instrument enter the Priority Buffers. Instead, a sample of trigger events is sent to the Priority Buffers, which are defined and weighted to target particle types according to the goals of the LET instrument. Priority Buffers (listed in Table 3.8 and described in detail elsewhere — **TBD**) are defined to identify classes of particles by penetration range, by charge or charge range, or by other characteristic (e.g. STIM events). There is some overlap in information between Particle ID and Priority Buffer number. The Priority Buffer definitions and the filling and extracting methods are described elsewhere (**TBD)**. See Section 3, Table 3.8 for a list of Priority Buffer numbers.

The L1A through L3B trigger tags identify which detector groups were involved in the trigger conditions, and the A/B tag identifies which side of the detector provided the trigger. The HAZ flag marks a hazard condition **TBD**. The STIM flag marks a calibration event defined in *Specification of Functional Test Modules and In-flight Calibration Routines for LET, STEREO-CIT-006.A*. STIM events follow a special format, described in Section 2.10.

The Time Tag (Latency) Bits duplicate the four least significant bits of the minutes field of an onboard clock (LET internal minute counter), as an indicator of event latency. When events are packaged and placed in priority buffers, these minutes bits are copied onto the ERH Latency Bits. Later, when the full Science Frame is packaged into CCSDS packets, the time of the assembly of the Science Frame is copied onto time fields in the CCSDS packet headers and onto the Minutes counter of MISCBITS (Section 2.8, and Table 3.2). Because the time that an event is popped off its priority buffer and placed into the Science Frame may be delayed by more than one minute after the event is first pushed onto the priority buffer, the Latency Bits for a given event may not correspond to the time that the event's Science Frame is assembled. It is up to the user of the data to determine what value of the latency bits precisely corresponds to times associated with given Science Frames. (Note: Previous versions of this document identified the Latency Bits – or Time Tag bits – as counting the age of the event, in minutes, relative to its Science Frame. Also, because the Latency Bits are the 4 least significant bits of a minutes field in a clock, the value of the Latency Bits cycles from 0 to 15 three times, followed by 0 to 11, over the course of an hour.)

For some classes of events, large numbers of detectors or ADCs in the LET instrument may be triggered and result in signals. The LET Data Format (Event Record Format) described herein is capable of returning events with the maximum of 54 ADC hits. Most of these events are unlikely to be sorted by the LET Matrices, but some fraction of them will be sent to the Event Buffer. For events with sufficiently large numbers of hit ADCs, not all ADCs will be included in the Event Record. The onboard software will determine the maximum number of ADC signals transmitted for each event (**TBD**). Bits 25–27 will count the number of ADCs in the event which are **not** included in the Event Record, with a saturation value of 7.

A separate number counting the ADCs **included** in the Event Record is not included in the Event Record Header. Instead, and End of Record (EOR) bit is employed in the ADC Field, described later in this section. Furthermore, LET has a VERBOSE mode in which both low gain and high gain signals from a given ADC may be transmitted. By relying on the EOR bit in the ADC Fields, the format allows for transmission of low and high gain signals for any given ADC, and the EOR bit itself is sufficient to mark the length of an Event Record.

An Extended Header flag (bit 29) marks the addition 2 bytes of header information, described in Section 2.11. A STIM block flag (bit 30) marks the addition 2 bytes of STIM block information to the header, described in Section 2.10. A final ADC culling flag (bit 31) marks the condition that one or more ADCs were culled by onboard software for the event. If culling mode is off, this bit is always zero.

Following the header are a number of ADC fields. Each ADC field will contain the following:

Table 2.3: ADC Field — Minimum Bit Allocations

|  |  |  |
| --- | --- | --- |
| **Data** | **# Bits** | **Note** |
| **ADC Signal** | 12 | 11 bits signal, 1 bit overflow |
| **ADC/Detector ID** | 6 | 54 detectors maximum |
| **Low/High gain** | 1 | 0 = low gain, 1 = high gain |
| **Last hit flag (End of Record, EOR)** | 1 | Set to 1 for the last ADC in an event, 0 for all other ADCs |

Thus, each ADC signal and identifier is encoded in 20 bits. Note that the End of Record (EOR) bit is 0 except when set to 1 for the last ADC Field in an event record. The detector ID is the same as the detector address, a list of which can be found with the singles rates table, Section 3, Table 3.4. The format of the ADC Field is given in Figure 2.3:




Figure 2.3: Event Record ADC Field. End of Record (EOR) and Gain bits are defined in Table 2.3.

The smallest event record (one event record header plus 2 ADC Fields) would be 72 bits long. A 3 ADC event would be 92 bits long. The event records will be padded by 4 bits for each event record with odd numbers of ADC Fields, allowing all event records to be aligned to byte boundaries. Table 2.4 and Figures 2.4–2.5 show some examples, with the Figures diagramming Event Records as 3 bytes wide for illustration only.

Table 2.4: Bit padding of Event Records.

|  |  |  |  |
| --- | --- | --- | --- |
| # ADC Fields | # bits without padding | Padding bits | # bytes with padding |
| 2 | 72 | 0 | 9 |
| 3 | 92 | 4 | 12 |
| 4 | 112 | 0 | 14 |
| 5 | 132 | 4 | 17 |
| 6 | 152 | 0 | 19 |
| 7 | 172 | 4 | 22 |




Figure 2.4: Event Record with 2 ADC Fields. Left to right is MSB to LSB, spanning 3 bytes.




Figure 2.5: Event Record with 3 ADC Fields. Left to right is MSB to LSB, spanning 3 bytes.

Note: In the event of a bit error, particularly in the End of Record (EOR) bit in the ADC field, it is possible that all subsequent events in the Event Buffer will be unreconstructible or, at the very least, very difficult to reconstruct. Such bit errors are expected to be extremely rare. Possible remedies in the Event Record format may include enforcing MISC word boundaries for the ADC Field, and forcing bit 23 (EOR bit) in such ADC Fields to be 0 except at EOR. The disadvantage of this approach is an increase in the length in bytes of some events. The increasing number of unused bits in each event record will reduce the number of events possible in an Event Buffer.

Given the sizes of the Event Records and the included 4 bit padding of odd-number ADC events, Table 2.5 summarizes the Event Buffer capacity and the Telemetry Rate for events of up to 7 ADCs:

Table 2.5: Event Buffer Capacity and Telemetry Rate

|  |  |  |
| --- | --- | --- |
| **# ADCs** | **Maximum # Events in Buffer** | **Telemetry Rate (events/sec)** |
| 2 | 303 | 5.1 |
| 3 | 227 | 3.8 |
| 4 | 195 | 3.3 |
| 5 | 160 | 2.7 |
| 6 | 143 | 2.4 |
| 7 | 124 | 2.1 |

Note that these estimates assume that the STIM Information Block (Section 2.10) and the Extended Header Block (Section 2.11) are not included in the event record.

**2.10 Event Buffer – STIM Events**

Bit 19 of the Event Record Header flags calibration, or STIM, events. These events include livetime STIM events and ADC STIM events. Both of these types of STIM events will be included in the Event Buffer, with different priorities and different (or unassigned) particle IDs. However, because they represent a different class of event than regular particles, it is anticipated that additional information may be needed for calibration and identification. Therefore, an additional 3-byte STIM Information Block is appended to the Event Record for STIM events, after the ADC fields and optional Extended Header block.

A two ADC STIM event is shown in Figure 2.6.




Figure 2.6: Event Record with 2 ADC Fields. Left to right is MSB to LSB, spanning 3 bytes. Optional Extended Header Block is also attached.

STIM events will be padded to fill out bytes in the same way that regular events are padded, at the end of the event record.

The STIM Information Block is appended after the Event Record Header if bit 30 of the ERH is set. The STIM information block contains a "seconds" counter, the DACLEVEL, and the DACCONFIGURATION. The seconds counter contains the second number within the accumulation minute of the LET Science Frame during which the STIM event was taken. For example, during normal mode operation, livetime STIM events are accumulated during the 0-8 second, 10-18 second, 20-28 second, etc. time intervals, while ADC STIM events are accumulated at the 9 second, 19 second, 29 second, etc. points. The DACLEVEL (0-31) and DACCONFIGURATION (0-14) indicate via tables in the LET onboard software what the DAC settings are for the STIM events and which ADCs are stimulated, respectively.

**The bit assignments are defined elsewhere.** The assumed arrangement of bits is shown in Figure 2.7.




Figure 2.7: STIM Information Block

**2.11 Extended Header Block**

If bit 29 of the Event Record Header is set, an additional two byte Extended Header Block (or Extended Information Block) is appended after the ERH and ADC fields and before an optional STIM Information Block (Section 2.10). This Extended Header Block contains additional information useful for diagnosing onboard software function and performance.

The Extended Header Block currently contains DEINDEX (9 bits) and EPINDEX (7 bits). DEINDEX is the delta-E axis matrix index generated by the onboard software to map the given event to a LET Matrix Map (see Appendix C). It has a value in the range 0-399. EPINDEX is the residual energy axis matrix index (E-prime) generated by the onboard software to map the given event to a LET Matrix Map, and it has a value in the range 0-127.




Figure 2.8: Extended Header Block

**3.0 LET Science Frame Format Summary**

Tables 3.1–3.16 summarize the LET Science Data Frame Format, viewing the LET Data Frame as a stream of numbered bytes (0-4159). Descriptions of the contents of the Science Frame are given in Section 2, but these tables provide the byte locations of data elements in the LET Science Frame.

Note that the Science/Foreground Rates tables are quite long and span multiple pages.

Table 3.1: LET Science Data Frame Header Summary

|  |  |  |
| --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** |
| 0 | 0 | Bits 6-7 = 00 (EM unit), 01 (FM1, ahead), 10 (FM2, behind)  Bits 0-5 = frame version number |
| 1 | 2 | # Bytes used in Frame (SFLEN) |
| 3 | 4 | LET Science Frame Checksum (SFCHECK) |

Table 3.2: Miscellaneous Bits, MISCBITS

|  |  |  |
| --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** |
| 5 | 5 | Bit 7 = CodeOK  Bits 3-6 = HeaterDutyCycle  Bit 2 = LeakConv  Bits 0-1 = DyThState |
| 6 | 6 | Minute (LET internal minute counter) |

Table 3.3: Livetime Counters, ERATES (names **TBD**)

|  |  |  |
| --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** |
| 7 | 8 | Livetime counter, Front End Electronics |
| 9 | 10 | # Triggers (NUMTRIG) |
| 11 | 12 | # Rejected Events (NUMREJECT) |
| 13 | 14 | # Accepted Events with PHA data (NUMACCPHA) |
| 15 | 16 | # Accepted Events without PHA data (NUMACCNPHA) |
| 17 | 18 | NUMTRIG.HAZ |
| 19 | 20 | NUMREJECT.HAZ |
| 21 | 22 | NUMACCPHA.HAZ |
| 23 | 24 | NUMACCNPHA.HAZ |

Table 3.4: Singles Rates, SNGRATES

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **# Bytes** | **Description** | **Detector Address** |
| 25 | 28 | 4 | L2A0, High and Low Gain | 0 |
| 29 | 32 | 4 | L2A1, High and Low Gain | 1 |
| 33 | 36 | 4 | L2A2, High and Low Gain | 2 |
| 37 | 40 | 4 | L2A3, High and Low Gain | 3 |
| 41 | 44 | 4 | L2A4, High and Low Gain | 4 |
| 45 | 48 | 4 | L2A5, High and Low Gain | 5 |
| 49 | 52 | 4 | L2A6, High and Low Gain | 6 |
| 53 | 56 | 4 | L2A7, High and Low Gain | 7 |
| 57 | 60 | 4 | L2A8, High and Low Gain | 8 |
| 61 | 64 | 4 | L2A9, High and Low Gain | 9 |
| 65 | 68 | 4 | L3Ai, High and Low Gain | 14 |
| 69 | 72 | 4 | L3Ao, High and Low Gain | 15 |
| 73 | 76 | 4 | L1A0a, High and Low Gain | 16 |
| 77 | 80 | 4 | L1A0b, High and Low Gain | 17 |
| 81 | 84 | 4 | L1A0c, High and Low Gain | 18 |
| 85 | 88 | 4 | L1A1a, High and Low Gain | 19 |
| 89 | 92 | 4 | L1A1b, High and Low Gain | 20 |
| 93 | 96 | 4 | L1A1c, High and Low Gain | 21 |
| 97 | 100 | 4 | L1A2a, High and Low Gain | 22 |
| 101 | 104 | 4 | L1A2b, High and Low Gain | 23 |
| 105 | 108 | 4 | L1A2c, High and Low Gain | 24 |
| 109 | 112 | 4 | L1A3a, High and Low Gain | 25 |
| 113 | 116 | 4 | L1A3b, High and Low Gain | 26 |
| 117 | 120 | 4 | L1A3c, High and Low Gain | 27 |
| 121 | 124 | 4 | L1A4a, High and Low Gain | 28 |
| 125 | 128 | 4 | L1A4b, High and Low Gain | 29 |
| 129 | 132 | 4 | L1A4c, High and Low Gain | 30 |
| 133 | 136 | 4 | L1B0a, High and Low Gain | 32 |
| 137 | 140 | 4 | L1B0b, High and Low Gain | 33 |
| 141 | 144 | 4 | L1B0c, High and Low Gain | 34 |
| 145 | 148 | 4 | L1B1a, High and Low Gain | 35 |
| 149 | 152 | 4 | L1B1b, High and Low Gain | 36 |
| 153 | 156 | 4 | L1B1c, High and Low Gain | 37 |
| 157 | 160 | 4 | L1B2a, High and Low Gain | 38 |
| 161 | 164 | 4 | L1B2b, High and Low Gain | 39 |
| 165 | 168 | 4 | L1B2c, High and Low Gain | 40 |
| 169 | 172 | 4 | L1B3a, High and Low Gain | 41 |
| 173 | 176 | 4 | L1B3b, High and Low Gain | 42 |
| 177 | 180 | 4 | L1B3c, High and Low Gain | 43 |
| 181 | 184 | 4 | L1B4a, High and Low Gain | 44 |
| 185 | 188 | 4 | L1B4b, High and Low Gain | 45 |
| 189 | 192 | 4 | L1B4c, High and Low Gain | 46 |
| 193 | 196 | 4 | L2B0, High and Low Gain | 48 |
| 197 | 200 | 4 | L2B1, High and Low Gain | 49 |
| 201 | 204 | 4 | L2B2, High and Low Gain | 50 |
| 205 | 208 | 4 | L2B3, High and Low Gain | 51 |
| 209 | 212 | 4 | L2B4, High and Low Gain | 52 |
| 213 | 216 | 4 | L2B5, High and Low Gain | 53 |
| 217 | 220 | 4 | L2B6, High and Low Gain | 54 |
| 221 | 224 | 4 | L2B7, High and Low Gain | 55 |
| 225 | 228 | 4 | L2B8, High and Low Gain | 56 |
| 229 | 232 | 4 | L2B9, High and Low Gain | 57 |
| 233 | 236 | 4 | L3Bi, High and Low Gain | 62 |
| 237 | 240 | 4 | L3Bo, High and Low Gain | 63 |

Table 3.5: Miscellaneous Rates, MISCRATES (**TBD**)

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **# Bytes** | **Description** |
| 241 | 250 | 10 | Miscellaneous instrument rates (**TBD**) |

Table 3.6: Event Processing Rates, EVPRATES

|  |  |  |
| --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** |
| 251 | 252 | NREAD (events read from event FIFO) |
| 253 | 254 | NHAZ ( events rejected for Hazard condition ) |
| 255 | 256 | NADCSTIM ( ADC-calibration STIM events ) |
| 257 | 258 | NODD ( odd events ) |
| 259 | 260 | NODDFIX ( fixed odd events ) |
| 261 | 262 | NMULTI ( events with multiple hits in relevant layers ) |
| 263 | 264 | NMULTIFIX ( fixed multi events ) |
| 265 | 266 | NBADTRAJ ( events rejected for inconsistent/bad trajectory ) |
| 267 | 268 | NL2 ( events sorted into L12 event category ) |
| 269 | 270 | NL3 ( events sorted into L123 event category ) |
| 271 | 272 | NPEN ( events sorted into PEN event category ) |
| 273 | 274 | NFORMAT ( events handled by the telemetry event formatter ) |
| 275 | 276 | NASIDE ( events the software assumed were Aside events ) |
| 277 | 278 | NBSIDE ( events the software assumed were Bside events ) |
| 279 | 280 | NERROR ( events that caused a processing error - should never happen ) |
| 281 | 282 | NBADTAGS (events with bad tags from onboard event-processing) |

Table 3.7: Coincidence Rates, COINRATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **# Bytes** | **Description** |
| 283 | 284 | 2 | L12A |
| 285 | 286 | 2 | L123A |
| 287 | 288 | 2 | PENA |
| 289 | 290 | 2 | spare |
| 291 | 292 | 2 | L12B |
| 293 | 294 | 2 | L123B |
| 295 | 296 | 2 | PENB |
| 297 | 298 | 2 | spare |
| 299 | 300 | 2 | PENA? |
| 301 | 302 | 2 | PENB? |
| 303 | 304 | 2 | 2TEL |
| 305 | 306 | 2 | ERRTAG |

Table 3.8: Priority Buffer Rates, BUFRATES

|  |  |  |
| --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** |
| 307 | 308 | PB #0 ADC-cal events |
| 309 | 310 | PB #1 Range 2, 3, or 4 events that fall into Z>=40 matrix box |
| 311 | 312 | PB #2 Range 2, 3, or 4 events that fall into 31<=Z<=39 matrix box |
| 313 | 314 | PB #3 Range 3 events that fall into 9<=Z<=30 matrix box, or any foreground box that is painted over it. |
| 315 | 316 | PB #4 Range 2 events that fall into 9<=Z<=30 matrix box, or any foreground box that is painted over it. |
| 317 | 318 | PB #5 Range 3 events that fall into the LiBeB, CNO, C, N, or O matrix boxes |
| 319 | 320 | PB #6 Range 2 events that fall into the LiBeB, CNO, C, N, or O matrix boxes |
| 321 | 322 | PB #7 Range 4 events that fall into the LiBeB, CNO, or 9<=Z<=30 matrix boxes, or any foreground matrix box from C thru Ni. |
| 323 | 324 | PB #8 Range 4 events that fall into the PEN\_Z>30 matrix box ("penetrating" or "Range 5" events) |
| 325 | 326 | PB #9 Matrix-sort Reject events, with L3 signal, Z>=3 |
| 327 | 328 | PB #10 Matrix-sort Reject events, with NO L3 signal, Z>=3 |
| 329 | 330 | PB #11 Range 3 events that fall into 3He matrix box |
| 331 | 332 | PB #12 Range 2 events that fall into 3He matrix box |
| 333 | 334 | PB #13 Range 4 events that fall into the PEN\_3<=Z<=30 matrix box ("penetrating" or "Range 5" events) |
| 335 | 336 | PB #14 Range 3 events that fall into the He background or 4He foreground matrix box |
| 337 | 338 | PB #15 Range 4 events that fall into any He matrix box |
| 339 | 340 | PB #16 Range 2 events that fall into the He background or 4He foreground matrix box |
| 341 | 342 | PB #17 Range 3 events that fall into any H matrix box |
| 343 | 344 | PB #18 Range 4 events that fall into any H matrix box |
| 345 | 346 | PB #19 Range 2 events that fall into any H matrix box |
| 347 | 348 | PB #20 Matrix-sort Reject events, with L3 signal, Z<3 |
| 349 | 350 | PB #21 Matrix-sort Reject events, with NO L3 signal, Z<3 |
| 351 | 352 | PB #22 Range 4 events that fall into the PEN\_H\_He matrix box ("penetrating" or "Range 5" events) |
| 353 | 354 | PB #23 Range 2, 3, or 4 events that fall into the "Backward" matrix box |
| 355 | 356 | PB #24 "Clean" Livetime STIM events (stim events that fall into a STIM matrix box) |
| 357 | 358 | PB #25 "Poor" Livetime STIM events (stim events that either fall outside a STIM matrix box, or are rejected because of multiple hits in a layer, etc.) |
| 359 | 360 | PB #26 ERROR - Onboard processing of the event was aborted due to an error. Occurs if the tag-bits of the event are invalid. Can also occur if the onboard processing reaches a point that it should never reach. |
| 361 | 362 | PB #27 Other - currently not used |
| 363 | 364 | PB #28 Spare |

Table 3.9: LET Science Data Frame, Range 2 (L1L2) Science/Foreground Rates, L2FGRATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** | **Particle ID** |
| 365 | 366 | H (1.0-1.8 MeV/nuc) | 0 |
| 367 | 368 | H (1.8-2.2 MeV/nuc) | 1 |
| 369 | 370 | H (2.2-2.7 MeV/nuc) | 2 |
| 371 | 372 | H (2.7-3.2 MeV/nuc) | 3 |
| 373 | 374 | H (3.2-3.6 MeV/nuc) | 4 |
| 375 | 376 | H (3.6-4.0 MeV/nuc) | 5 |
| 377 | 378 | H (4.0-4.5 MeV/nuc) | 6 |
| 379 | 380 | H (4.5-5.0 MeV/nuc) | 7 |
| 381 | 382 | H (5.0-70.0 MeV/nuc) | 8 |
| 383 | 384 | He-3 (1.0-2.2 MeV/nuc) | 9 |
| 385 | 386 | He-3 (2.2-2.7 MeV/nuc) | 10 |
| 387 | 388 | He-3 (2.7-3.2 MeV/nuc) | 11 |
| 389 | 390 | He-3 (3.2-3.6 MeV/nuc) | 12 |
| 391 | 392 | He-3 (3.6-4.0 MeV/nuc) | 13 |
| 393 | 394 | He-3 (4.0-4.5 MeV/nuc) | 14 |
| 395 | 396 | He-3 (4.5-5.0 MeV/nuc) | 15 |
| 397 | 398 | He-3 (5.0-6.0 MeV/nuc) | 16 |
| 399 | 400 | He-3 (6.0-70.0 MeV/nuc) | 17 |
| 401 | 402 | He-4 (1.0-1.8 MeV/nuc) | 18 |
| 403 | 404 | He-4 (1.8-2.2 MeV/nuc) | 19 |
| 405 | 406 | He-4 (2.2-2.7 MeV/nuc) | 20 |
| 407 | 408 | He-4 (2.7-3.2 MeV/nuc) | 21 |
| 409 | 410 | He-4 (3.2-3.6 MeV/nuc) | 22 |
| 411 | 412 | He-4 (3.6-4.0 MeV/nuc) | 23 |
| 413 | 414 | He-4 (4.0-4.5 MeV/nuc) | 24 |
| 415 | 416 | He-4 (4.5-5.0 MeV/nuc) | 25 |
| 417 | 418 | He-4 (5.0-70.0 MeV/nuc) | 26 |
| 419 | 420 | C (1.0-3.2 MeV/nuc) | 27 |
| 421 | 422 | C (3.2-3.6 MeV/nuc) | 28 |
| 423 | 424 | C (3.6-4.0 MeV/nuc) | 29 |
| 425 | 426 | C (4.0-4.5 MeV/nuc) | 30 |
| 427 | 428 | C (4.5-5.0 MeV/nuc) | 31 |
| 429 | 430 | C (5.0-6.0 MeV/nuc) | 32 |
| 431 | 432 | C (6.0-8.0 MeV/nuc) | 33 |
| 433 | 434 | C (8.0-10.0 MeV/nuc) | 34 |
| 435 | 436 | C (10.0-70.0 MeV/nuc) | 35 |
| 437 | 438 | N (1.0-3.2 MeV/nuc) | 36 |
| 439 | 440 | N (3.2-3.6 MeV/nuc) | 37 |
| 441 | 442 | N (3.6-4.0 MeV/nuc) | 38 |
| 443 | 444 | N (4.0-4.5 MeV/nuc) | 39 |
| 445 | 446 | N (4.5-5.0 MeV/nuc) | 40 |
| 447 | 448 | N (5.0-6.0 MeV/nuc) | 41 |
| 449 | 450 | N (6.0-8.0 MeV/nuc) | 42 |
| 451 | 452 | N (8.0-10.0 MeV/nuc) | 43 |
| 453 | 454 | N (10.0-70.0 MeV/nuc) | 44 |
| 455 | 456 | O (1.0-3.2 MeV/nuc) | 45 |
| 457 | 458 | O (3.2-3.6 MeV/nuc) | 46 |
| 459 | 460 | O (3.6-4.0 MeV/nuc) | 47 |
| 461 | 462 | O (4.0-4.5 MeV/nuc) | 48 |
| 463 | 464 | O (4.5-5.0 MeV/nuc) | 49 |
| 465 | 466 | O (5.0-6.0 MeV/nuc) | 50 |
| 467 | 468 | O (6.0-8.0 MeV/nuc) | 51 |
| 469 | 470 | O (8.0-10.0 MeV/nuc) | 52 |
| 471 | 472 | O (10.0-70.0 MeV/nuc) | 53 |
| 473 | 474 | Ne (1.0-3.2 MeV/nuc) | 54 |
| 475 | 476 | Ne (3.2-3.6 MeV/nuc) | 55 |
| 477 | 478 | Ne (3.6-4.0 MeV/nuc) | 56 |
| 479 | 480 | Ne (4.0-4.5 MeV/nuc) | 57 |
| 481 | 482 | Ne (4.5-5.0 MeV/nuc) | 58 |
| 483 | 484 | Ne (5.0-6.0 MeV/nuc) | 59 |
| 485 | 486 | Ne (6.0-8.0 MeV/nuc) | 60 |
| 487 | 488 | Ne (8.0-10.0 MeV/nuc) | 61 |
| 489 | 490 | Ne (10.0-12.0 MeV/nuc) | 62 |
| 491 | 492 | Ne (12.0-70.0 MeV/nuc) | 63 |
| 493 | 494 | Mg (1.0-3.2 MeV/nuc) | 64 |
| 495 | 496 | Mg (3.2-3.6 MeV/nuc) | 65 |
| 497 | 498 | Mg (3.6-4.0 MeV/nuc) | 66 |
| 499 | 500 | Mg (4.0-4.5 MeV/nuc) | 67 |
| 501 | 502 | Mg (4.5-5.0 MeV/nuc) | 68 |
| 503 | 504 | Mg (5.0-6.0 MeV/nuc) | 69 |
| 505 | 506 | Mg (6.0-8.0 MeV/nuc) | 70 |
| 507 | 508 | Mg (8.0-10.0 MeV/nuc) | 71 |
| 509 | 510 | Mg (10.0-12.0 MeV/nuc) | 72 |
| 511 | 512 | Mg (12.0-15.0 MeV/nuc) | 73 |
| 513 | 514 | Mg (15.0-70.0 MeV/nuc) | 74 |
| 515 | 516 | Si (1.0-3.2 MeV/nuc) | 75 |
| 517 | 518 | Si (3.2-3.6 MeV/nuc) | 76 |
| 519 | 520 | Si (3.6-4.0 MeV/nuc) | 77 |
| 521 | 522 | Si (4.0-4.5 MeV/nuc) | 78 |
| 523 | 524 | Si (4.5-5.0 MeV/nuc) | 79 |
| 525 | 526 | Si (5.0-6.0 MeV/nuc) | 80 |
| 527 | 528 | Si (6.0-8.0 MeV/nuc) | 81 |
| 529 | 530 | Si (8.0-10.0 MeV/nuc) | 82 |
| 531 | 532 | Si (10.0-12.0 MeV/nuc) | 83 |
| 533 | 534 | Si (12.0-15.0 MeV/nuc) | 84 |
| 535 | 536 | Si (15.0-70.0 MeV/nuc) | 85 |
| 537 | 538 | S (1.0-3.6 MeV/nuc) | 86 |
| 539 | 540 | S (3.6-4.0 MeV/nuc) | 87 |
| 541 | 542 | S (4.0-4.5 MeV/nuc) | 88 |
| 543 | 544 | S (4.5-5.0 MeV/nuc) | 89 |
| 545 | 546 | S (5.0-6.0 MeV/nuc) | 90 |
| 547 | 548 | S (6.0-8.0 MeV/nuc) | 91 |
| 549 | 550 | S (8.0-10.0 MeV/nuc) | 92 |
| 551 | 552 | S (10.0-12.0 MeV/nuc) | 93 |
| 553 | 554 | S (12.0-15.0 MeV/nuc) | 94 |
| 555 | 556 | S (15.0-70.0 MeV/nuc) | 95 |
| 557 | 558 | Ar (1.0-3.6 MeV/nuc) | 96 |
| 559 | 560 | Ar (3.6-4.0 MeV/nuc) | 97 |
| 561 | 562 | Ar (4.0-4.5 MeV/nuc) | 98 |
| 563 | 564 | Ar (4.5-5.0 MeV/nuc) | 99 |
| 565 | 566 | Ar (5.0-6.0 MeV/nuc) | 100 |
| 567 | 568 | Ar (6.0-8.0 MeV/nuc) | 101 |
| 569 | 570 | Ar (8.0-10.0 MeV/nuc) | 102 |
| 571 | 572 | Ar (10.0-12.0 MeV/nuc) | 103 |
| 573 | 574 | Ar (12.0-15.0 MeV/nuc) | 104 |
| 575 | 576 | Ar (15.0-21.0 MeV/nuc) | 105 |
| 577 | 578 | Ar (21.0-70.0 MeV/nuc) | 106 |
| 579 | 580 | Ca (1.0-3.6 MeV/nuc) | 107 |
| 581 | 582 | Ca (3.6-4.0 MeV/nuc) | 108 |
| 583 | 584 | Ca (4.0-4.5 MeV/nuc) | 109 |
| 585 | 586 | Ca (4.5-5.0 MeV/nuc) | 110 |
| 587 | 588 | Ca (5.0-6.0 MeV/nuc) | 111 |
| 589 | 590 | Ca (6.0-8.0 MeV/nuc) | 112 |
| 591 | 592 | Ca (8.0-10.0 MeV/nuc) | 113 |
| 593 | 594 | Ca (10.0-12.0 MeV/nuc) | 114 |
| 595 | 596 | Ca (12.0-15.0 MeV/nuc) | 115 |
| 597 | 598 | Ca (15.0-21.0 MeV/nuc) | 116 |
| 599 | 600 | Ca (21.0-70.0 MeV/nuc) | 117 |
| 601 | 602 | Fe (1.0-2.7 MeV/nuc) | 118 |
| 603 | 604 | Fe (2.7-3.2 MeV/nuc) | 119 |
| 605 | 606 | Fe (3.2-3.6 MeV/nuc) | 120 |
| 607 | 608 | Fe (3.6-4.0 MeV/nuc) | 121 |
| 609 | 610 | Fe (4.0-4.5 MeV/nuc) | 122 |
| 611 | 612 | Fe (4.5-5.0 MeV/nuc) | 123 |
| 613 | 614 | Fe (5.0-6.0 MeV/nuc) | 124 |
| 615 | 616 | Fe (6.0-8.0 MeV/nuc) | 125 |
| 617 | 618 | Fe (8.0-10.0 MeV/nuc) | 126 |
| 619 | 620 | Fe (10.0-12.0 MeV/nuc) | 127 |
| 621 | 622 | Fe (12.0-15.0 MeV/nuc) | 128 |
| 623 | 624 | Fe (15.0-21.0 MeV/nuc) | 129 |
| 625 | 626 | Fe (21.0-70.0 MeV/nuc) | 130 |
| 627 | 628 | Na, Al, Ni, unidentified | 255 |

Table 3.10: LET Science Data Frame, Range 2 (L1L2) Science/Background Rates, L2BGRATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** | **Particle ID** |
| 629 | 630 | H Background | 255 |
| 631 | 632 | He Background | 255 |
| 633 | 634 | LiBeB Background | 255 |
| 635 | 636 | CNO Background | 255 |
| 637 | 638 | Z=9-30 Background | 255 |
| 639 | 640 | Z=30-40 Background | 255 |
| 641 | 642 | Z>=40 Background | 255 |
| 643 | 644 | Backward Background | 255 |
| 645 | 646 | H, He STIM | 255 |
| 647 | 648 | CNO STIM | 255 |
| 649 | 650 | Fe STIM | 255 |
| 651 | 652 | STIM error | 255 |

Table 3.11: LET Science Data Frame, Range 3 (L2L3) Science/Foreground Rates, L3FGRATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** | **Particle ID** |
| 653 | 654 | H (1.0-3.2 MeV/nuc) | 0 |
| 655 | 656 | H (3.2-3.6 MeV/nuc) | 1 |
| 657 | 658 | H (3.6-4.0 MeV/nuc) | 2 |
| 659 | 660 | H (4.0-4.5 MeV/nuc) | 3 |
| 661 | 662 | H (4.5-5.0 MeV/nuc) | 4 |
| 663 | 664 | H (5.0-6.0 MeV/nuc) | 5 |
| 665 | 666 | H (6.0-8.0 MeV/nuc) | 6 |
| 667 | 668 | H (8.0-10.0 MeV/nuc) | 7 |
| 669 | 670 | H (10.0-12.0 MeV/nuc) | 8 |
| 671 | 672 | H (12.0-15.0 MeV/nuc) | 9 |
| 673 | 674 | H (15.0-70.0 MeV/nuc) | 10 |
| 675 | 676 | He-3 (1.0-4.0 MeV/nuc) | 11 |
| 677 | 678 | He-3 (4.0-4.5 MeV/nuc) | 12 |
| 679 | 680 | He-3 (4.5-5.0 MeV/nuc) | 13 |
| 681 | 682 | He-3 (5.0-6.0 MeV/nuc) | 14 |
| 683 | 684 | He-3 (6.0-8.0 MeV/nuc) | 15 |
| 685 | 686 | He-3 (8.0-10.0 MeV/nuc) | 16 |
| 687 | 688 | He-3 (10.0-12.0 MeV/nuc) | 17 |
| 689 | 690 | He-3 (12.0-15.0 MeV/nuc) | 18 |
| 691 | 692 | He-3 (15.0-70.0 MeV/nuc) | 19 |
| 693 | 694 | He-4 (1.0-3.2 MeV/nuc) | 20 |
| 695 | 696 | He-4 (3.2-3.6 MeV/nuc) | 21 |
| 697 | 698 | He-4 (3.6-4.0 MeV/nuc) | 22 |
| 699 | 700 | He-4 (4.0-4.5 MeV/nuc) | 23 |
| 701 | 702 | He-4 (4.5-5.0 MeV/nuc) | 24 |
| 703 | 704 | He-4 (5.0-6.0 MeV/nuc) | 25 |
| 705 | 706 | He-4 (6.0-8.0 MeV/nuc) | 26 |
| 707 | 708 | He-4 (8.0-10.0 MeV/nuc) | 27 |
| 709 | 710 | He-4 (10.0-12.0 MeV/nuc) | 28 |
| 711 | 712 | He-4 (12.0-15.0 MeV/nuc) | 29 |
| 713 | 714 | He-4 (15.0-70.0 MeV/nuc) | 30 |
| 715 | 716 | C (1.0-4.5 MeV/nuc) | 31 |
| 717 | 718 | C (4.5-5.0 MeV/nuc) | 32 |
| 719 | 720 | C (5.0-6.0 MeV/nuc) | 33 |
| 721 | 722 | C (6.0-8.0 MeV/nuc) | 34 |
| 723 | 724 | C (8.0-10.0 MeV/nuc) | 35 |
| 725 | 726 | C (10.0-12.0 MeV/nuc) | 36 |
| 727 | 728 | C (12.0-15.0 MeV/nuc) | 37 |
| 729 | 730 | C (15.0-21.0 MeV/nuc) | 38 |
| 731 | 732 | C (21.0-27.0 MeV/nuc) | 39 |
| 733 | 734 | C (27.0-33.0 MeV/nuc) | 40 |
| 735 | 736 | C (33.0-70.0 MeV/nuc) | 41 |
| 737 | 738 | N (1.0-5.0 MeV/nuc) | 42 |
| 739 | 740 | N (5.0-6.0 MeV/nuc) | 43 |
| 741 | 742 | N (6.0-8.0 MeV/nuc) | 44 |
| 743 | 744 | N (8.0-10.0 MeV/nuc) | 45 |
| 745 | 746 | N (10.0-12.0 MeV/nuc) | 46 |
| 747 | 748 | N (12.0-15.0 MeV/nuc) | 47 |
| 749 | 750 | N (15.0-21.0 MeV/nuc) | 48 |
| 751 | 752 | N (21.0-27.0 MeV/nuc) | 49 |
| 753 | 754 | N (27.0-33.0 MeV/nuc) | 50 |
| 755 | 756 | N (33.0-70.0 MeV/nuc) | 51 |
| 757 | 758 | O (1.0-5.0 MeV/nuc) | 52 |
| 759 | 760 | O (5.0-6.0 MeV/nuc) | 53 |
| 761 | 762 | O (6.0-8.0 MeV/nuc) | 54 |
| 763 | 764 | O (8.0-10.0 MeV/nuc) | 55 |
| 765 | 766 | O (10.0-12.0 MeV/nuc) | 56 |
| 767 | 768 | O (12.0-15.0 MeV/nuc) | 57 |
| 769 | 770 | O (15.0-21.0 MeV/nuc) | 58 |
| 771 | 772 | O (21.0-27.0 MeV/nuc) | 59 |
| 773 | 774 | O (27.0-33.0 MeV/nuc) | 60 |
| 775 | 776 | O (33.0-70.0 MeV/nuc) | 61 |
| 777 | 778 | Ne (1.0-6.0 MeV/nuc) | 62 |
| 779 | 780 | Ne (6.0-8.0 MeV/nuc) | 63 |
| 781 | 782 | Ne (8.0-10.0 MeV/nuc) | 64 |
| 783 | 784 | Ne (10.0-12.0 MeV/nuc) | 65 |
| 785 | 786 | Ne (12.0-15.0 MeV/nuc) | 66 |
| 787 | 788 | Ne (15.0-21.0 MeV/nuc) | 67 |
| 789 | 790 | Ne (21.0-27.0 MeV/nuc) | 68 |
| 791 | 792 | Ne (27.0-33.0 MeV/nuc) | 69 |
| 793 | 794 | Ne (33.0-40.0 MeV/nuc) | 70 |
| 795 | 796 | Ne (40.0-70.0 MeV/nuc) | 71 |
| 797 | 798 | Na (1.0-6.0 MeV/nuc) | 72 |
| 799 | 800 | Na (6.0-8.0 MeV/nuc) | 73 |
| 801 | 802 | Na (8.0-10.0 MeV/nuc) | 74 |
| 803 | 804 | Na (10.0-12.0 MeV/nuc) | 75 |
| 805 | 806 | Na (12.0-15.0 MeV/nuc) | 76 |
| 807 | 808 | Na (15.0-21.0 MeV/nuc) | 77 |
| 809 | 810 | Na (21.0-27.0 MeV/nuc) | 78 |
| 811 | 812 | Na (27.0-33.0 MeV/nuc) | 79 |
| 813 | 814 | Na (33.0-40.0 MeV/nuc) | 80 |
| 815 | 816 | Na (40.0-70.0 MeV/nuc) | 81 |
| 817 | 818 | Mg (1.0-6.0 MeV/nuc) | 82 |
| 819 | 820 | Mg (6.0-8.0 MeV/nuc) | 83 |
| 821 | 822 | Mg (8.0-10.0 MeV/nuc) | 84 |
| 823 | 824 | Mg (10.0-12.0 MeV/nuc) | 85 |
| 825 | 826 | Mg (12.0-15.0 MeV/nuc) | 86 |
| 827 | 828 | Mg (15.0-21.0 MeV/nuc) | 87 |
| 829 | 830 | Mg (21.0-27.0 MeV/nuc) | 88 |
| 831 | 832 | Mg (27.0-33.0 MeV/nuc) | 89 |
| 833 | 834 | Mg (33.0-40.0 MeV/nuc) | 90 |
| 835 | 836 | Mg (40.0-52.0 MeV/nuc) | 91 |
| 837 | 838 | Mg (52.0-70.0 MeV/nuc) | 92 |
| 839 | 840 | Al (1.0-6.0 MeV/nuc) | 93 |
| 841 | 842 | Al (6.0-8.0 MeV/nuc) | 94 |
| 843 | 844 | Al (8.0-10.0 MeV/nuc) | 95 |
| 845 | 846 | Al (10.0-12.0 MeV/nuc) | 96 |
| 847 | 848 | Al (12.0-15.0 MeV/nuc) | 97 |
| 849 | 850 | Al (15.0-21.0 MeV/nuc) | 98 |
| 851 | 852 | Al (21.0-27.0 MeV/nuc) | 99 |
| 853 | 854 | Al (27.0-33.0 MeV/nuc) | 100 |
| 855 | 856 | Al (33.0-40.0 MeV/nuc) | 101 |
| 857 | 858 | Al (40.0-52.0 MeV/nuc) | 102 |
| 859 | 860 | Al (52.0-70.0 MeV/nuc) | 103 |
| 861 | 862 | Si (1.0-6.0 MeV/nuc) | 104 |
| 863 | 864 | Si (6.0-8.0 MeV/nuc) | 105 |
| 865 | 866 | Si (8.0-10.0 MeV/nuc) | 106 |
| 867 | 868 | Si (10.0-12.0 MeV/nuc) | 107 |
| 869 | 870 | Si (12.0-15.0 MeV/nuc) | 108 |
| 871 | 872 | Si (15.0-21.0 MeV/nuc) | 109 |
| 873 | 874 | Si (21.0-27.0 MeV/nuc) | 110 |
| 875 | 876 | Si (27.0-33.0 MeV/nuc) | 111 |
| 877 | 878 | Si (33.0-40.0 MeV/nuc) | 112 |
| 879 | 880 | Si (40.0-52.0 MeV/nuc) | 113 |
| 881 | 882 | Si (52.0-70.0 MeV/nuc) | 114 |
| 883 | 884 | S (1.0-6.0 MeV/nuc) | 115 |
| 885 | 886 | S (6.0-8.0 MeV/nuc) | 116 |
| 887 | 888 | S (8.0-10.0 MeV/nuc) | 117 |
| 889 | 890 | S (10.0-12.0 MeV/nuc) | 118 |
| 891 | 892 | S (12.0-15.0 MeV/nuc) | 119 |
| 893 | 894 | S (15.0-21.0 MeV/nuc) | 120 |
| 895 | 896 | S (21.0-27.0 MeV/nuc) | 121 |
| 897 | 898 | S (27.0-33.0 MeV/nuc) | 122 |
| 899 | 900 | S (33.0-40.0 MeV/nuc) | 123 |
| 901 | 902 | S (40.0-52.0 MeV/nuc) | 124 |
| 903 | 904 | S (52.0-70.0 MeV/nuc) | 125 |
| 905 | 906 | Ar (1.0-6.0 MeV/nuc) | 126 |
| 907 | 908 | Ar (6.0-8.0 MeV/nuc) | 127 |
| 909 | 910 | Ar (8.0-10.0 MeV/nuc) | 128 |
| 911 | 912 | Ar (10.0-12.0 MeV/nuc) | 129 |
| 913 | 914 | Ar (12.0-15.0 MeV/nuc) | 130 |
| 915 | 916 | Ar (15.0-21.0 MeV/nuc) | 131 |
| 917 | 918 | Ar (21.0-27.0 MeV/nuc) | 132 |
| 919 | 920 | Ar (27.0-33.0 MeV/nuc) | 133 |
| 921 | 922 | Ar (33.0-40.0 MeV/nuc) | 134 |
| 923 | 924 | Ar (40.0-52.0 MeV/nuc) | 135 |
| 925 | 926 | Ar (52.0-70.0 MeV/nuc) | 136 |
| 927 | 928 | Ca (1.0-8.0 MeV/nuc) | 137 |
| 929 | 930 | Ca (8.0-10.0 MeV/nuc) | 138 |
| 931 | 932 | Ca (10.0-12.0 MeV/nuc) | 139 |
| 933 | 934 | Ca (12.0-15.0 MeV/nuc) | 140 |
| 935 | 936 | Ca (15.0-21.0 MeV/nuc) | 141 |
| 937 | 938 | Ca (21.0-27.0 MeV/nuc) | 142 |
| 939 | 940 | Ca (27.0-33.0 MeV/nuc) | 143 |
| 941 | 942 | Ca (33.0-40.0 MeV/nuc) | 144 |
| 943 | 944 | Ca (40.0-52.0 MeV/nuc) | 145 |
| 945 | 946 | Ca (52.0-70.0 MeV/nuc) | 146 |
| 947 | 948 | Fe (1.0-8.0 MeV/nuc) | 147 |
| 949 | 950 | Fe (8.0-10.0 MeV/nuc) | 148 |
| 951 | 952 | Fe (10.0-12.0 MeV/nuc) | 149 |
| 953 | 954 | Fe (12.0-15.0 MeV/nuc) | 150 |
| 955 | 956 | Fe (15.0-21.0 MeV/nuc) | 151 |
| 957 | 958 | Fe (21.0-27.0 MeV/nuc) | 152 |
| 959 | 960 | Fe (27.0-33.0 MeV/nuc) | 153 |
| 961 | 962 | Fe (33.0-40.0 MeV/nuc) | 154 |
| 963 | 964 | Fe (40.0-52.0 MeV/nuc) | 155 |
| 965 | 966 | Fe (52.0-70.0 MeV/nuc) | 156 |
| 967 | 968 | Ni (1.0-8.0 MeV/nuc) | 157 |
| 969 | 970 | Ni (8.0-10.0 MeV/nuc) | 158 |
| 971 | 972 | Ni (10.0-12.0 MeV/nuc) | 159 |
| 973 | 974 | Ni (12.0-15.0 MeV/nuc) | 160 |
| 975 | 976 | Ni (15.0-21.0 MeV/nuc) | 161 |
| 977 | 978 | Ni (21.0-27.0 MeV/nuc) | 162 |
| 979 | 980 | Ni (27.0-33.0 MeV/nuc) | 163 |
| 981 | 982 | Ni (33.0-40.0 MeV/nuc) | 164 |
| 983 | 984 | Ni (40.0-52.0 MeV/nuc) | 165 |
| 985 | 986 | Ni (52.0-70.0 MeV/nuc) | 166 |

Table 3.12: LET Science Data Frame, Range 3 (L2L3) Science/Background Rates, L3BGRATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** | **Particle ID** |
| 987 | 988 | H Background | 255 |
| 989 | 990 | He Background | 255 |
| 991 | 992 | LiBeB Background | 255 |
| 993 | 994 | CNO Background | 255 |
| 995 | 996 | Z=9-30 Background | 255 |
| 997 | 998 | Z=30-40 Background | 255 |
| 999 | 1000 | Z>=40 Background | 255 |
| 1001 | 1002 | Backward Background | 255 |
| 1003 | 1004 | H, He STIM | 255 |
| 1005 | 1006 | CNO STIM | 255 |
| 1007 | 1008 | Fe STIM | 255 |
| 1009 | 1010 | STIM error | 255 |

Table 3.13: LET Science Data Frame, Range 4 (L3AL3B) Science/Foreground Rates, PENFGRATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** | **Particle ID** |
| 1011 | 1012 | H (1.0-12.0 MeV/nuc) | 0 |
| 1013 | 1014 | H (12.0-15.0 MeV/nuc) | 1 |
| 1015 | 1016 | H (15.0-70.0 MeV/nuc) | 2 |
| 1017 | 1018 | He-4 (1.0-12.0 MeV/nuc) | 3 |
| 1019 | 1020 | He-4 (12.0-15.0 MeV/nuc) | 4 |
| 1021 | 1022 | He-4 (15.0-70.0 MeV/nuc) | 5 |
| 1023 | 1024 | C (1.0-21.0 MeV/nuc) | 6 |
| 1025 | 1026 | C (21.0-27.0 MeV/nuc) | 7 |
| 1027 | 1028 | C (27.0-33.0 MeV/nuc) | 8 |
| 1029 | 1030 | C (33.0-70.0 MeV/nuc) | 9 |
| 1031 | 1032 | N (1.0-21.0 MeV/nuc) | 10 |
| 1033 | 1034 | N (21.0-27.0 MeV/nuc) | 11 |
| 1035 | 1036 | N (27.0-33.0 MeV/nuc) | 12 |
| 1037 | 1038 | N (33.0-70.0 MeV/nuc) | 13 |
| 1039 | 1040 | O (1.0-27.0 MeV/nuc) | 14 |
| 1041 | 1042 | O (27.0-33.0 MeV/nuc) | 15 |
| 1043 | 1044 | O (33.0-70.0 MeV/nuc) | 16 |
| 1045 | 1046 | Ne (1.0-27.0 MeV/nuc) | 17 |
| 1047 | 1048 | Ne (27.0-33.0 MeV/nuc) | 18 |
| 1049 | 1050 | Ne (33.0-40.0 MeV/nuc) | 19 |
| 1051 | 1052 | Ne (40.0-70.0 MeV/nuc) | 20 |
| 1053 | 1054 | Mg (1.0-33.0 MeV/nuc) | 21 |
| 1055 | 1056 | Mg (33.0-40.0 MeV/nuc) | 22 |
| 1057 | 1058 | Mg (40.0-52.0 MeV/nuc) | 23 |
| 1059 | 1060 | Mg (52.0-70.0 MeV/nuc) | 24 |
| 1061 | 1062 | Si (1.0-33.0 MeV/nuc) | 25 |
| 1063 | 1064 | Si (33.0-40.0 MeV/nuc) | 26 |
| 1065 | 1066 | Si (40.0-52.0 MeV/nuc) | 27 |
| 1067 | 1068 | Si (52.0-70.0 MeV/nuc) | 28 |
| 1069 | 1070 | Fe (1.0-40.0 MeV/nuc) | 29 |
| 1071 | 1072 | Fe (40.0-52.0 MeV/nuc) | 30 |
| 1073 | 1074 | Fe (52.0-70.0 MeV/nuc) | 31 |
| 1075 | 1076 | He-3, Na, Al, S, Ar, Ca, Ni, Unidentified | 255 |

Table 3.14: LET Science Data Frame, Range 4 (L3AL3B) Science/Background Rates, PENBGRATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** | **Particle ID** |
| 1077 | 1078 | H Background | 255 |
| 1079 | 1080 | He Background | 255 |
| 1081 | 1082 | LiBeB Background | 255 |
| 1083 | 1084 | CNO Background | 255 |
| 1085 | 1086 | Z=9-30 Background | 255 |
| 1087 | 1088 | Z=30-40 Background | 255 |
| 1089 | 1090 | Z>=40 Background | 255 |
| 1091 | 1092 | Backward Background | 255 |
| 1093 | 1094 | H, He PEN | 255 |
| 1095 | 1096 | Z=3-30 PEN | 255 |
| 1097 | 1098 | Z>30 PEN | 255 |
| 1099 | 1100 | H, He STIM | 255 |
| 1101 | 1102 | CNO STIM | 255 |
| 1103 | 1104 | Fe STIM | 255 |
| 1105 | 1106 | STIM error | 255 |

Table 3.15: LET Science Data Frame, Look Direction/Sectored Rates, SECTRATES

|  |  |  |  |
| --- | --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **# Bytes** | **Description** |
| 1107 | 1122 | 16 | H, 4-6 MeV, Side A (Look Directions 0-7) |
| 1123 | 1138 | 16 | H, 4-6 MeV, Side B (Look Directions 8-15) |
| 1139 | 1154 | 16 | He-3, 4-6 MeV/nuc, Side A (Look Directions 0-7) |
| 1155 | 1170 | 16 | He-3, 4-6 MeV/nuc, Side B (Look Directions 8-15) |
| 1171 | 1186 | 16 | He-4, 4-6 MeV/nuc, Side A (Look Directions 0-7) |
| 1187 | 1202 | 16 | He-4, 4-6 MeV/nuc, Side B (Look Directions 8-15) |
| 1203 | 1218 | 16 | He-4, 6-12 MeV/nuc, Side A (Look Directions 0-7) |
| 1219 | 1234 | 16 | He-4, 6-12 MeV/nuc, Side B (Look Directions 8-15) |
| 1235 | 1250 | 16 | CNO, 4-6 MeV/nuc, Side A (Look Directions 0-7) |
| 1251 | 1266 | 16 | CNO, 4-6 MeV/nuc, Side B (Look Directions 8-15) |
| 1267 | 1282 | 16 | CNO, 6-12 MeV/nuc, Side A (Look Directions 0-7) |
| 1283 | 1298 | 16 | CNO, 6-12 MeV/nuc, Side B (Look Directions 8-15) |
| 1299 | 1314 | 16 | NeMgSi, 4-6 MeV/nuc, Side A (Look Directions 0-7) |
| 1315 | 1330 | 16 | NeMgSi, 4-6 MeV/nuc, Side B (Look Directions 8-15) |
| 1331 | 1346 | 16 | NeMgSi, 6-12 MeV/nuc, Side A (Look Directions 0-7) |
| 1347 | 1362 | 16 | NeMgSi, 6-12 MeV/nuc, Side B (Look Directions 8-15) |
| 1363 | 1378 | 16 | Fe, 4-6 MeV/nuc, Side A (Look Directions 0-7) |
| 1379 | 1394 | 16 | Fe, 4-6 MeV/nuc, Side B (Look Directions 8-15) |
| 1395 | 1410 | 16 | Fe, 6-12 MeV/nuc, Side A (Look Directions 0-7) |
| 1411 | 1426 | 16 | Fe, 6-12 MeV/nuc, Side B (Look Directions 8-15) |

Table 3.16: LET Science Data Frame, Event Buffer

|  |  |  |
| --- | --- | --- |
| **Frame Byte # (First)** | **Frame Byte # (Last)** | **Description** |
| 1427 | 1428 | Event Buffer Header (# Event Records) |
| 1429 | 4159 | Event Records (filled as needed) |

**Appendix A: Rates Compression/Decompression Algorithm**

The following algorithms were suggested in an e-mail from Don Reames, for compressing 32 bits to 16 bits. This finalized algorithm is a modified biased exponent, hidden one algorithm with a 12 bit mantissa and a 4 bit exponent. Numbers up to 212 are uncompressed, and numbers up to 213 decompress with no “error”.

/\* Rewrite to allow flexible arrangements of bits. AWL 030909 \*/

unsigned int num\_bits=16, num\_mantissa\_bits=12, num\_exponent\_bits=4;

unsigned long output\_mask=0xffff; /\* 0xffff 16 bit, 0x0fff 12 bit \*/

/\* 32-bit -> 16-bit compression for SW and HW rates \*/

/\* useage: rateout=pack\_rate(ratein); \*/

unsigned int pack\_rate(ratein)

long ratein;

{

unsigned int rateout, power=0;

unsigned long mask;

mask = (0xffffffff<<(num\_mantissa\_bits+1));

while (ratein&mask)

{

power += (0x0001<<num\_mantissa\_bits);

ratein>>=1;

}

rateout=ratein;

if (power)

{

rateout = power + (0x0001<<num\_mantissa\_bits)

| (rateout & (output\_mask>>num\_exponent\_bits));

}

rateout = (rateout & output\_mask);

return rateout;

}

/\* Unpacking (not required in flight code) \*/

/\* switched from long to unsigned long -- AWL 011107 \*/

unsigned long long\_rate(packed) /\* Unpack to long \*/

unsigned long packed; /\* was just long. AWL 030908 \*/

{

unsigned long power; /\* was just long. AWL 030908 \*/

unsigned long out; /\* was just long. AWL 030908 \*/

power = packed>>num\_mantissa\_bits;

if (power>1)

{

out = ( (packed & (output\_mask>>num\_exponent\_bits))

| (0x0001<<num\_mantissa\_bits) );

out = out<<(power-1);

}

else

out = packed;

return out;

}

double dbl\_rate(packed) /\* Unpack to double \*/

unsigned packed;

{

int power;

double out;

power = packed>>num\_mantissa\_bits;

if (power>1)

{

out = ( (packed & (output\_mask>>num\_exponent\_bits))

| (0x0001<<num\_mantissa\_bits) );

out = out \* pow(2.,(double)(power-1));

}

else

out = packed;

return out;

}

**Appendix B: Outstanding Issues**

* Verify checksum algorithm.
* Define event sampling algorithm here or point to definition in some other document (e.g. is it already in *STEREO-CIT-002.F STEREO SEP LET and SEP Central Flight Software Requirements*?).
* Need formal documentation for livetimes, Event Processing Counters, and Priority Buffer Counters, and their uses. Priority Buffers are set out in RAM memos, and Event Processing Counters are listed in *LET Software Counter Definitions* (*STEREO-CIT-019.A*). Documentation should be entered in the STEREO/LET Documentation catalog. (Section 2.7.)
* Misc. Rates need to be defined. (Section 2.8).
* Define hazard condition for HAZ flag in Event Record Header.
* Set maximum number of ADCs to be included in Event Records, and define the ADC selection criteria when the number of hit ADCs passes the maximum. Didn't we already do this?
* Verify STIM information block format for STIM Event Record Headers.
* Verify Extended Header format..

**Appendix C: LET Matrices**

The LET Matrices are used in onboard processing for identifying particles by penetration range, element, and energy, using the delta–E vs. E’ technique. The matrices and their use in the onboard software are documented elsewhere. However, for purposes of illustration, graphical representations of the matrices are included in this Appendix.

The matrices are 128 bins (x–axis) by 400 bins (y–axis), mapped over delta–E vs E’ space. Each bin contains a number identifying either a “foreground” particle (selected elements or helium isotopes) or a “background” particle. Colors in the figures are assigned according to the bin value, but the colors are not unique to the bin values. Rather, light orange, red, and green were selected to contrast adjacent foreground tracks, and shades of blue and purple were selected to contrast adjacent background regions. The white (uncolored) region bounds backward–going particles, and STIM boxes are bright orange.

Solid yellow and dashed green lines center and outline the particle tracks for selected elements and helium isotopes. The curves were calculated using the Andersen and Ziegler (1977) range–energy relationship, assuming normal incidence through the LET detectors. The points are simulation data (M. Wiedenbeck, run 050).

The Matrices represented by the following plots are at Version 8e.




Figure C.1: The Range 2 (L1 vs. L2, or L1L2) LET matrix. Foreground elements are H, He-3, He-4, C, N, O, Ne, Mg, Si, S, Ar, Ca, and Fe.




Figure C.2: The Range 3 (L2 vs. L3, or L2L3) LET matrix. Foreground elements are H, He-3, He-4, C, N, O, Ne, Na, Mg, Al, Si, S, Ar, Ca, Fe, and Ni.




Figure C.3: The Range 4 (L3A vs. L3B, or L3AL3B) LET matrix. Foreground elements are H, He-4, C, N, O, Ne, Mg, Si, and Fe. The dark diagonal regions mark penetrating particles (or RNG 5).

**Appendix D: Version History**

1.0

Original

1.1

In version 1.0, we assumed 6 energy bins and 3 species bins (H, He3, and He4), with 16 bits per lo-res rate. These assumptions yielded 36 bytes of lo-res rates per LET Science Frame. These were increased to 4 energy bins for H and 5 species bins and 8 energy bins for He, or a total of 88 bytes of lo-res rates per LET Science Frame.

In version 1.0, we assumed 8 energy bins and 7 species (C, N, O, Ne, Mg, Si, and Fe), also with 16 bits per rate. These assumptions yield 112 bytes, divided among 15 LET Science Frames, for 7-8 bytes per frame. Assume 8 bytes per frame, with the 15th frame having a blank 8 bytes which can be used for other data, such as lo-res diagnostics.

In version 1.0, there were 44 detector segments, requiring 6 bits for detector IDs. In version 1.1, there are now 54 detector segments, with L1 detectors now having two outer ring segments instead of one. However, only 6 bits are still required.

2.0

Add LET Science Frame Header.

Add LET Science Frame Format Summary Table.

Add note about possible bit errors in the Event Buffer. This may require further revision.

3.0

Switch lo-res rates to hi-res rates — consolidate all rates. “1 minute for H, He; 15 minutes for Z≥6” becomes “1 minute for all species”. Given that the rates are now no longer divided into low and high resolution rates, the 15 minute cycle is now eliminated. Lo-res and hi-res rates are now designated as science rates (or species).

Switch rates to 16 bits, log-compressed.

4.0

Add appendix showing compression/decompression code.

Update bit rate allocation (or LET Science Frame size) for LET, up to 16 CCSDS packets/minute.

Reduce data transmission rate to once every 3 seconds.

Add K, Ar, and make Mg be in 3 charge bins.

Fix # species in Table 1.

Add look direction.

4.1

Removed minor frame structure, replacing minor frames with full CCSDS packets.

4.2

Add HAZ and STIM bits (replacing default 0’s) to event record headers.

5.0

Migrate master document to Microsoft Word X for Mac OS X format (from Appleworks 6).

Remove reference to Phase A Study Report; it is superceded by more recent documentation and discussion.

Add singles rates.

There is now a single byte checksum at the end of each CCSDS packet, which takes away an additional byte per CCSDS packet.

Modified frame header to include count of # CCSDS packets and # bytes in frame.

Rewrite Event Record Header to eliminate L1 vs. L2+L3 index (obsolete), add Good/Bad flag and # hits and # adcs.

6.0

Add sections on byte order, ApIDs.

Change singles rates to include both low and high gain singles rates – doubling the number of singles rates and eating into the Event Buffer.

Rewrite section on TBD undetermined space and change it to housekeeping space.

Add special STIM event format.

Switch to 4 bit exponent in compression algorithm.

Various corrections to errors in the text.

7.0

Update references to STEREO-CIT-002.F from version E.

Add reference to STEREO-CIT-007.F.

Remove Ne isotopes as a requirement from Table 1. It is still a goal.

Add a spacecraft/source/version ID byte to the header – this despite the fact that spacecraft id will be on all packets or somesuch according to Dave Curtis. (Section 2.3)

Correct an error in the byte numbering in the LET Science Frame Header (Section 2.3).

Corrected an error in the text of Section 2.6 which stated that there will be 60 singles and coincidence rates. Tables 17 is correct.

Define a numbering scheme for the look direction sectors.

Add livetime definitions to the housekeeping. (See Appendix B – do we need a DPU livetime?)

Fixed a bunch of table reference errors.

Added extra information to the format summary tables.

Rename Appendix B (this appendix) as Appendix C, and insert a new Appendix B for “outstanding issues”.

Modified compression algorithm to 12 bit mantissa, 4 bit exponent. (Appendix A.)

Slightly modified definition of Particle ID (Section 2.4) to match the fact that the Event Record Header (Section 2.8) now assigns only 8 bits instead of 9 (in version 6).

Updated the Event Record Header to the final result from discussions and e–mails around September 11, 2003. Also updated text with event record header discussion.

Added look direction definitions, and inserted a new table 7.

Switched the order of charge bin and energy columns in Tables 3-6, to reflect the now-explicit ordering by range, element, charge bin, and energy in the text. (I may have swapped charge bin and energy ordering when I previously discussed this with Bob Radocinski.) This ordering reflects the way the L1L2, etc. matrices will be straightened out to species vs. energy, so that ordering will first be along the y-axes (element, charge) then along the x-axes (energy).

Added revised livetimes. Note that livetime counters now take up 130 bytes, filling the housekeeping section.

8.0

Extensive rewrite based on software meeting of 1/8/04.

Rewrite goals (Table 1) to drop Ne and Mg isotopes — no longer possible with 128x400 LET Matrices. Only He-3 and He-4 isotopes are in rates data.

P. 1: The 11 byte header and 1 byte checksum for each 272 byte CCSDS packet are not included in the LET Science Data Frame Format.

Rewrote Section 2.2 ApIDs. A single ApID (580) is assigned to the entire frame. Individual packets are numbered in the subsecond field bits of the CCSDS packet headers.

Added Section 2.10, Miscellaneous Bits and Rates (TBD).

Remove references to isotopes other than He-3 and He-4 throughout this document. The LET rate matrices will not accomodate Ne and Mg isotopes as of this version.

Appendix C (Version History) now shifted to Appendix D, and Appendix C inserted for LET Matrices.

Renumber tables in X.Y form, where X is section number. Fixed figure numbering as well.

In Section 2.9 (formerly Section 2.8), 2nd paragraph, the 438 2-ADC events in the buffer space is in error, left over from version 4 of this document, in which the Event Buffer was 3506 bytes long. Update this number, finally, to the correct value of ~303 for the current format.

Expand the Event Record Header format to 4 bytes based on R. Mewaldt’s memo of 10/23/03 and A. Davis’ e–mail of 1/21/04, adding the addition byte to the header and swapping the order of STIM and HAZ bits.

Updated a lot of numbers, including # events per frame.

9.0

Swap byte order (section 2.1) to high byte first. Correct example in Section 2.1 to reflect 4 bytes in event record header.

Swap byte order of table columns in Section 3.

Modify Figures 2.4, 2.5, and 2.6 to reflect the new byte order.

Change text in a couple of spots to reflect the new byte order.

Replace column headings “Frame Byte # (Low)” and “Frame Byte # (High)” in Section 3 with “Frame Byte # (First)” and “Frame Byte # (Last)” in order to avoid confusion, since data elements are transmitted high byte first.

Expand time tag (Latency tag in ERH) to four bits, and modify table 2.2 and figure 2.2 accordingly. Insert blurb about extended header, missing from previous version.

10.0

Named coincidence rates, and added 2 “spare” coincidence rates.

Fixed text error on p. 3. Rates occupy ~5.5 packets, not ~4.5 packets.

10.1

Fixed naming of NUMACCPHA and NUMACCNPHA in Table 3.3.

11.0

"Elements to be resolved or to be determined, or elements documented only in software, are marked **TBD" to acknowledge a lot of software already written but not documented here or likely elsewhere.**

Section 2: The LET Science Data Frame Format will now "attempt to" accommodate goals listed in Table 1.1. Some telemetry goals may be affected by the inclusion of optional information blocks in event records.

Science Frame Byte 0 (Science Frame Header, section 2.3) now gives the two most significant bits to identify the EM unit, FM1, and FM2. The remaining bits are still the LET Science Frame Version (#11).

Section 2.8: MISCBITS are now defined, at least with software tag names. I don't have documentation on the functions. MISCRATES are still left blank as of this version.

Defined bits 30 (STIM block flag) and 31 (culling flag) in the Event Record Header (ERH), Table 2.2, Section 2.9. Also updated Figure 2.2.

Section 2.10: Fixed figure 2.6 for a 3 byte STIM information block. The figure originally showed a 2-byte block. Added information on the STIM information block, as extracted from Bob Radocinski's letevent\_\_define.pro code. However, the exact arrangement of bits can't be determined from that code, so this information is imprecise at this moment.

Added Section 2.11 Extended Header Block. I assume it's 2 bytes and contains only DEINDEX and EPINDEX, based on Bob Radocinski's software, but as with the STIM information block, I'm not sure of the precise configuration.

Section 3.0, updated tables 3.1, 3.2, 3.6,3.8, 3.9, 3.11, 3.13, and 3.15.

Updated matrix plots (Appendix C) to version 6.

12.0

After e-mail discussion I had with Andrew Davis and Bob Radocinski, we determined that the onboard software doesn't match the format of the event record as described in version 11 of this document. In the software, the Extended Header block and STIM information block come after the ADC fields, and the extended header block is 16 bits. Bit padding (to fill out to byte boundaries) occurs at the end of the event record, after the optional blocks. Changed Figures 2.6 and 2.7 to match the format, and changed the t ext as needed (and where I found the text to be incorrect – some errors may yet remain).

Added some description of hardware counters to Section 2.7.

12.1

Section 2.2: Fixed error so that bits 0-3 of the subseconds field of the CCSDS packet header are replaced by the packet number (0-15), not bits 0-4. Was versin 12.0 in error? Or did we eventually allocate 5 bits in case we'd get to use 20 CCSDS packets?

13.0

Section 2.9 and Table 2.2: Fixed the definition and discussion of Latency Bits, based on analysis and discussions from the January 2007 time when I had thought that latency might provide a hint as to why Priority Buffer 24 was suddenly showing low count rates, as well as documentation detective work by MEW on 4/9/07. The Latency Bits are the 4 least significant bits of the minutes counter in MISCBITS. See my 1/18/07 e-mail and whatever else we sent around at that time; the data I plotted were on the Behind spacecraft, from 2007\_017\_1\_05. (The problem was eventually traced to misplaced pointers onboard.) The new definition is also the same as that in the instrument paper, but in more detail.

Updated matrix plots (Appendix C) to Version 8e.

8/30/07: Added "Time Tag" to "Latency Bits" in a couple of places.

###### LET Geometry Factors

Note: these are nominal geometry factors. The calibration files used in Level 1 data processing may contain slightly different (updated) values.

